# UPPER SIDE

This section describes the names and functions of the respective parts inside the machine.
×
Toner cartridge
This cartridge contains toner.
When the toner in a cartridge runs out, replace with new one.
- REPLACEMENT OF TONER CARTRIDGE
×
Fusing unit
Heat is applied here to fuse the transferred image onto the paper.
The fusing unit is hot. Take care not to burn yourself when removing a misfeed.
×
Transfer roller
The black toner image is transferred onto the transfer roller.
Do not touch or damage the transfer roller.
This may cause a defective image.
×
Right side cover
Open this cover to remove a misfeed.
×
Paper reversing section cover
This unit is used for reversing paper when 2-sided printing is performed. Open this cover to remove a paper misfeed.
×
Main power switch
Use this switch to turn on the power for the machine.
When using the fax or Internet fax functions, always keep this switch in the “” position.
- TURNING ON THE POWER
×
Toner collection container
This container collects excess toner that remains after printing.
- REPLACING THE TONER COLLECTION CONTAINER
A service technician collects replaced toner collection containers.
×
Toner collection container release lever
Press up this lever when you need to release the toner collection container lock to replace the toner collection container.
- REPLACING THE TONER COLLECTION CONTAINER
×
Handle
Pull this out and grasp it when moving the machine.
×
Paper tray right side cover
Open this to remove a paper misfeed in tray 1 or 2.
×
Right side cover release lever
To remove a paper misfeed, pull and hold this lever up to open the right side cover.
×
Bypass tray
Use this tray to feed paper manually.
When loading paper larger than A4R or 8-1/2" x 11"R, pull out the extension guide.
- LOADING PAPER INTO THE BYPASS TRAY
×
A stand/500/2x500/3x500/500&2000 sheet paper drawer right-side cover
Open this cover to remove a paper misfeed in tray 2, 3 or 4.
Tap the name to make its details pop up. Back to top