# TEMPORARILY CHANGING THE SENDER INFORMATION(OWN NAME SELECT)

## Overview

You can temporarily change sender information to be used in the own number sending by selecting from data stored separately.
The function is released when the transmission with the changed sender information ends.

###### To store the sender information to be used for Own Name Select function:

In "Setting mode (administrator)", select [System Settings] → [Image Send Settings] → [Operation Settings] → [Own Name and Destination Set] → [Registration of Own Name Select].

## Operation

Place the original.
Place the original in the document feeder tray of the automatic document feeder, or on the document glass.

- AUTOMATIC DOCUMENT FEEDER
- DOCUMENT GLASS

Specify the destination fax number.

- ENTERING A DESTINATION NUMBER USING THE NUMERIC KEYS
- RETRIEVING A DESTINATION NUMBER FROM AN ADDRESS BOOK
- THE SELECTED DESTINATIONS
- USING A SEARCH NUMBER TO RETRIEVE A DESTINATION
- RETRIEVING A DESTINATION NUMBER FROM A GLOBAL ADDRESS BOOK
- USING A TRANSMISSION LOG TO RESEND
- SENDING BY CHAIN DIALLING

Tap the [Others] key, and tap the [Own Name Select] key.
Tap the sender information key to specify the sender information used for own number sending.
After the settings are completed, tap .
To cancel the sender information settings:
Tap the [Clear] key.
Tap the [Start] key to start scanning of the original.

- If you inserted the original pages in the document feeder tray, all pages are scanned.
  A beep will sound to indicate that scanning has ended, and the machine stands by for transmission.
- If you placed the original on the document glass, scan each page one at a time.
  When scanning finishes, place the next original and tap the [Start] key. Repeat until all pages have been scanned and then tap the [Read-End] key.
  A beep will sound to indicate that scanning has ended, and the machine stands by for transmission.

Tap the [Preview] key to preview the output image before sending it. After you have scanned an original by tapping the [Preview] key, tap the [Additional Scan] key to scan the next original. Tap the [Start] key to start sending an image.
For more information, see "CHECKING THE IMAGE TO BE TRANSMITTED". However, settings for this function cannot be changed in the preview screen.
Back to top