# CONFIDENTIAL TRANSMISSION USING F-CODES

## Overview

Send a fax to a destination fax number after adding the F-code (sub-address and passcode).
If necessary, the F-code confidential transmission can be used in combination with a broadcast transmission or timer transmission. It is convenient to store this function in a program.
The F-code confidential transmission cannot be registered as a "favourite" item.

## Operation

Place the original.
Place the original in the document feeder tray of the automatic document feeder, or on the document glass.

- AUTOMATIC DOCUMENT FEEDER
- DOCUMENT GLASS

Specify the destination.

1. (1) Enter the destination line number using the numeric keys.
2. (2) Tap the [Sub Address] key.
   Symbol "/" is entered.
3. (3) Enter the sub-address using the numeric keys.
4. (4) Tap the [Passcode] key.
   Symbol "/" is entered.
5. (5) Enter the passcode using the numeric keys.

- If the sub-address and passcode are already registered, you can select a one-touch key as well.
- If the passcode is omitted for the memory box of destination machine, you can skip Steps (4) and (5).
Tap the [Start] key.
Scanning of the original starts.

- If you inserted the original pages in the document feeder tray, all pages are scanned.
  A beep will sound to indicate that scanning and transmission have ended.
- If you placed the original on the document glass, scan each page one at a time.
  When scanning finishes, place the next original and tap the [Start] key. Repeat until all pages have been scanned and then tap the [Read-End] key.
  A beep will sound to indicate that transmission has ended.

Tap the [Preview] key to preview the output image before sending it. After you have scanned an original by tapping the [Preview] key, tap the [Additional Scan] key to scan the next original. Tap the [Start] key to start sending an image.
For more information, see "CHECKING THE IMAGE TO BE TRANSMITTED". However, settings for this function cannot be changed in the preview screen.
Back to top