# SENDING A THIN ORIGINAL(SLOW SCAN MODE)

## Overview

Use this function when you wish to scan thin originals using the automatic document feeder. This function helps prevent thin originals from misfeeding.
When slow scan mode is selected, 2-sided scanning is not possible.

## Operation

Place the original in the document feeder tray of the automatic document feeder.

- AUTOMATIC DOCUMENT FEEDER

Adjust the original guides slowly.
If the originals are inserted with too much force, they may crumple and misfeed.
Enter the destination fax number.

- ENTERING A DESTINATION NUMBER USING THE NUMERIC KEYS
- RETRIEVING A DESTINATION NUMBER FROM AN ADDRESS BOOK
- THE SELECTED DESTINATIONS
- USING A SEARCH NUMBER TO RETRIEVE A DESTINATION
- RETRIEVING A DESTINATION NUMBER FROM A GLOBAL ADDRESS BOOK
- USING A TRANSMISSION LOG TO RESEND
- SENDING BY CHAIN DIALLING

Tap the [Slow Scan Mode] key.
A checkmark appears on the icon.
To cancel the Slow Scan Mode setting:
Tap the [Slow Scan Mode] key to clear the checkmark.
Tap the [Start] key to start scanning of the original.
A beep will sound to indicate that scanning and transmission have ended.
Tap the [Preview] key to preview the output image before sending it. After you have scanned an original by tapping the [Preview] key, tap the [Additional Scan] key to scan the next original. Tap the [Start] key to start sending an image.
For more information, see "CHECKING THE IMAGE TO BE TRANSMITTED". However, settings for this function cannot be changed in the preview screen.
Back to top