# SENDING BOTH SIDES OF A CARD AS A SINGLE PAGE(CARD SHOT)

## Overview

Send the front and reverse sides of a card as a single page, without the need to send each side separately.
When using this function, the original must be placed on the document glass.

- If the original size is larger than the send size, it will result in a sending failure. Check the original size once more, and specify it again.
- The ratio cannot be specified and "Rotation Sending Setting" cannot be selected.
- This function cannot be used in direct transmission mode or when the speaker is used to dial.

## Operation

Place a card face down on the document glass.

- DOCUMENT GLASS

Enter the destination fax number.

- ENTERING A DESTINATION NUMBER USING THE NUMERIC KEYS
- RETRIEVING A DESTINATION NUMBER FROM AN ADDRESS BOOK
- THE SELECTED DESTINATIONS
- USING A SEARCH NUMBER TO RETRIEVE A DESTINATION
- RETRIEVING A DESTINATION NUMBER FROM A GLOBAL ADDRESS BOOK
- USING A TRANSMISSION LOG TO RESEND
- SENDING BY CHAIN DIALLING

Tap the [Others] key, and tap the [Card Shot] key.
Tap the [On] key, and specify the original size as required.

- Tap the areas displaying width and height sizes respectively, and enter the sizes using the numeric keys.
- To quickly set the size, first specify a value close to the desired ratio value by the numeric keys, then adjust it by tapping .

After the settings are completed, tap and [Back] keys in sequence.

- To enlarge or reduce the images to fit the paper based on the entered original size, set the [Fit to Send Size] checkbox to .
- After selecting Card Shot, tap the [Original] key in the base screen to change the original scan size or the send size. In this case, the screen of this step appears when you tap the scan size key. For the procedure for setting the send size, see "SPECIFYING THE SEND SIZE OF THE IMAGE".

To cancel the Card Shot settings:
Tap the [Off] key.
Tap the [Start] key, and scan the front side.
Tap the [Preview] key to check the preview of an image before sending a fax. For more information, see "CHECKING THE IMAGE TO BE TRANSMITTED".
However, settings for this function cannot be changed in the preview screen.
Place a card face up on the document glass, and tap the [Start] key to scan the reverse side.
Before scanning the back of the card, tap the [Change Setting] key on the touch panel to change the exposure.
Tap the [Read-End] key.
If you will continue by scanning the front of the card, you can tap the [Change Setting] key to change the exposure, resolution, scan size, and send size.
Back to top