# FAX TRANSMISSION SEQUENCE

First, tap the [Fax] icon on the home screen to enter fax mode.

- SELECTING FAX MODE

Place the original.
Place the original in the document feeder tray of the automatic document feeder, or on the document glass.

- AUTOMATIC DOCUMENT FEEDER
- DOCUMENT GLASS

Enter the destination fax number.
Tap the numeric keys to enter the destination number directly, or search and retrieve the address book or number.

- ENTERING A DESTINATION NUMBER USING THE NUMERIC KEYS
- RETRIEVING A DESTINATION NUMBER FROM AN ADDRESS BOOK
- THE SELECTED DESTINATIONS
- USING A SEARCH NUMBER TO RETRIEVE A DESTINATION
- RETRIEVING A DESTINATION NUMBER FROM A GLOBAL ADDRESS BOOK
- USING A TRANSMISSION LOG TO RESEND
- SENDING BY CHAIN DIALLING

Configure the scan settings.
Specify the original scan size, exposure, resolution, etc.

- IMAGE SETTINGS

If necessary, you can refer to the following functions for the setting.

- SENDING ORIGINALS COLLECTIVELY
- SCANNING ORIGINALS

- AUTOMATICALLY SCANNING BOTH SIDES OF AN ORIGINAL(2-SIDED ORIGINAL)
- AUTO DETECTION
- SPECIFYING THE ORIGINAL SCAN SIZE IN PAPER SIZE
- SPECIFYING THE ORIGINAL SCAN SIZE USING NUMERIC VALUES
- SPECIFYING THE SEND SIZE OF THE IMAGE
- CHANGING THE EXPOSURE
- CHANGING THE RESOLUTION
- SENDING A LARGE NUMBER OF PAGES(JOB BUILD)
- SENDING A THIN ORIGINAL(SLOW SCAN MODE)
- SENDING ORIGINALS OF DIFFERENT SIZES(MIXED SIZE ORIGINAL)
- CHECKING THE NUMBER OF SCANNED ORIGINAL SHEETS BEFORE TRANSMISSION(ORIGINAL COUNT)

Set Others.
Use Others other than the time when using scan settings such as sending two pages as a single page or sending originals of different sizes at the same time.
Send the original.
Tap the [Start] key.
- You can check the preview image by tapping the [Preview] key before tapping the [Start] key. After you have scanned an original by tapping the [Preview] key, tap the [Additional Scan] key to scan the next original.
- If you tap the [File] key or [Quick File] key on the action panel before starting fax transmission, you can save the scanned original as data.

- QUICK FILE
- FILE

When the original is placed on the document glass:

- If you placed the original on the document glass, carry out the following procedure to send a fax.

- When sending a fax normally (memory transmission)
  Repeat the steps for placing and scanning the originals the same number of times as there are originals. After scanning all originals, tap the [Read-End] key. (After you have scanned an original by tapping the [Preview] key, tap the [Additional Scan] key to scan the next original. Then, tap the [Start] key to send the original.)
- When sending a fax in direct transmission mode
  Multi-page originals cannot be scanned in direct transmission mode. Tap the [Start] key to start transmission.

- When sending a fax in direct transmission mode
  Multiple originals cannot be scanned in direct transmission mode. Tap the [Start] key to start transmission.

Back to top