# INTERNET FAX SETTINGS

The Internet Fax functions can be set.
Receive Settings
Internet fax reception
Enables the Internet fax reception functions.
POP3 Server
Enter the IP address or host name of the POP3 server.
Port Number
Enter the port number of the POP3 server. The default setting is port 110.
POP Authentication
The authentication protocol (including APOP) is used for authentication to the POP3 server.
User Name
Enter the user name. The special user account is required for Internet fax reception.
Password
Enter the password.
To change the password, select [Change Password] and enter the new password in the text box.
POP3 Communication Timeout
Set a timeout for communication to the POP3 server.
Reception Check Interval Setting
Enter an acknowledge cycle to the POP3 server.
Enable SSL
Allows the POP over SSL communication or the POP over TLS communication by STLS command. This requires the server to support the POP over SSL communication or the STLS command.
To allow the POP over SSL communication, set the "Port Number" to the POP over SSL communication port number.
To allow POP over TLS communication, set the "Port Number" to the same port number as for the normal POP3 communication.
Connection Test
Tap the [Execute] button to test the connection to the POP3 server.
Default Settings
I-Fax Own Name and Address Set
Set these options to store the sender name and source address to be used for Internet fax communication. The stored sender name and source address will be printed at the top of the received fax.
Sender Name
Enter the default sender name.
I-Fax Own Address
Enter the default source address.
Direct SMTP Settings
Port Number (Receive)
Enter the receive port number for direct SMTP communication. The default setting is port 25.
Timeout
Enter a timeout.
Port Number (Send)
Enter the transmit port number for direct SMTP communication. The default setting is port 25.
Timeout
Enter a timeout.
Back to top