# STAMPING SCANNED ORIGINALS(VERIFICATION STAMP)

## Overview

This function stamps each original that is scanned using the automatic document feeder, allowing you to verify that all originals were correctly scanned.

- To use the verification stamp function, the optional stamp unit must be installed.
- When 2-sided originals are used, the front of each original is stamped twice.
- If an error occurs during scanning, an original that was not scanned may be stamped.
- When the "O" mark that is stamped on originals starts to become faint, replace the stamp cartridge.
  For the procedure for replacing the stamp cartridge, see "REPLACING THE STAMP CARTRIDGE".

## Operation

Place originals in the automatic document feeder.

- AUTOMATIC DOCUMENT FEEDER

Specify the destination.

- RETRIEVING A DESTINATION FROM AN ADDRESS BOOK
- VIEWING A LIST OF THE SELECTED DESTINATIONS
- USING A SEARCH NUMBER TO RETRIEVE A DESTINATION
- ENTERING AN ADDRESS MANUALLY
- SPECIFYING A NETWORK FOLDER
- RETRIEVING A DESTINATION FROM A GLOBAL ADDRESS BOOK
- USING A TRANSMISSION LOG TO RESEND

Tap the [Verification Stamp] key on the action panel or [Others] key, and tap the [Verification Stamp] key.
The appropriate icon or checkbox is selected.
If you tap the [Others] key, tap the [Back] key after the settings have been completed.
To cancel the Verification Stamp setting:
Tap the [Verification Stamp] key on the action panel or [Others] key, and tap the [Verification Stamp] key to clear the checkmark.
Tap the [Start] key to start scanning of the original.
Tap the [Preview] key to check the preview of an image before sending a fax. For more information, see "CHECKING THE IMAGE TO BE TRANSMITTED". However, settings for this function cannot be changed in the preview screen.
A beep will sound to indicate that scanning and transmission have ended.
Back to top