# REPLACING THE TONER CARTRIDGE

## Overview

When toner is running low, the message prompting you to replace the toner cartridge appears.
You should keep one set of replacement toner cartridges on hand so that you can replace a toner cartridge immediately when toner runs out.
Replacement message
When toner is running low, the message "Toner Low (Do not replace cartridge until requested)" appears. When this message appears, prepare a toner cartridge for replacement.
When the amount of toner decreases further, the message "Ready to scan for copy. (Change the toner cartridge.)" appears. When this message appears, replace the toner cartridge.
When the toner runs out, printing is stopped and the message "Change the toner cartridge." appears.

If you continue to use the machine without replacing the cartridge, the following message will appear. Once the machine enters this state, printing cannot be carried out until the toner cartridge is replaced.

- Do not throw a toner cartridge into a fire. Toner may fly and cause burns.
- Store toner cartridges out of reach of small children.
- If a toner cartridge is stored on end, the toner may harden and become unusable. Always store toner cartridges on their side.
- If a toner cartridge other than a SHARP-recommended toner cartridge is used, the machine may not attain full quality and performance and there is a risk of damage to the machine. Be sure to use a SHARP-recommended toner cartridge.

Depending on your conditions of use, the colour may become light or the image blurred.

- Keep used toner cartridges in a plastic bag (do not discard them). Your service technician will collect used toner cartridges.
- To view the approximate amount of toner remaining (indicated in %), hold down the [Home Screen] button during printing or in standby mode.
- When toner runs out while the home screen is displayed, the [Toner Empty] message appears in the upper right corner of the screen.

## Operation

Open the front cover.
Pull the toner cartridge toward you.
Gently pull out the toner cartridge horizontally.
If the cartridge is pulled out abruptly, toner may spill out.
Hold the toner cartridge with both hands as shown and slowly pull it out of the machine.
Take out a new toner cartridge from its package and shake it five or six times.
Slowly insert the new toner cartridge on the level.
Push the cartridge in until it locks securely in place.
Keep pushing in the cartridge until it clicks into place.
Close the front cover.
After the toner cartridge is replaced, the machine automatically enters image adjustment mode. Do not open the front cover while this is occurring.
Back to top