# USING A TRANSMISSION LOG TO RESEND

## Overview

Select a destination from a transmission log and resend the data.
The destinations of the most recent 50 transmissions by fax, Scan to E-mail, and/or Internet fax are stored. One of these can be selected to resend to that destination. The destinations of the FTP/Desktop transmission and Scan to Network Folder are also shown in the transmission log.
The addresses shown in the transmission log can also be stored in an address book. This is a convenient way to store the fax numbers and addresses of destinations that were manually entered. However, addresses of the FTP/Desktop/Network Folder transmission cannot be stored from the machine.

- If numeric keys were tapped during the previous transmission, the number may not be redialled correctly.
- The fax addresses below are not stored as addresses for which resend is possible.
  - One-touch key for a contact or group in which multiple destinations are stored.
  - Broadcasting destinations
  - Destinations transmitted to using a program

## Operation

Tap the [Select among addresses recently sent to] key on the action panel.
Tap the key of the fax destination that you wish to redial.
The last 50 addresses used for transmission are displayed.
To cancel the resend setting:
Tap the highlighted key.
When you select the destination and tap the [Register New Address in Address Book], the destination can be stored in the address book. This is convenient if you have entered a destination directly.
Back to top