# FINISHER (LARGE STACKER)

## Overview

This device outputs sorted paper while staggering each set of paper. As needed, it staples each set. To punch holes in printed paper, install an optional hole punch module.

- Function names
- Supplies
- Finisher (large stacker) maintenance

Function names
×
Output tray (upper tray, lower tray)
Stapled and offset output is delivered to this tray.
The tray is slidable. Extend the tray for printing on large-size paper (A3W, A3, B4, 12" x 18", 11" x 17", 8-1/2" x 14" and 8-1/2" x 13" sizes).
×
Top cover
Open this cover to remove a paper misfeed.
×
Staple compiler
This temporarily stacks paper to be stapled.
×
Front cover
Open this cover to replace the staple cartridge or remove a staple jam.
Tap the name to make its details pop up.

- A paper pass unit is required to install a finisher (large stacker) as well as a stand/500/2x500/3x500/500&2000 sheet paper drawer.
- Do not place heavy objects on the finisher (large stacker) or press down on the finisher (large stacker).
- A finisher (large stacker) cannot be installed simultaneously with a finisher, saddle finisher or saddle finisher (large stacker).
- Exercise caution when you turn on the power and when printing is taking place, as the output tray may move up and down.

Supplies
The finisher (large stacker) requires the following staple cartridge:
Staple cartridge (approx. 5000 staples per cartridge x three cartridges)
AR-SC2
Finisher (large stacker) maintenance
When the staple cartridge runs out of staples, a message will appear in the operation panel. Follow the operation procedure to replace the staple cartridge.

## Operation

### Replacing the cartridge

Open the front cover.
Squeeze the green parts of the staple case and pull the case up and then out.
Remove the empty staple cartridge.
Press the lock button to release the staple case cover and then remove the staple cartridge.
When staples remain, the staple cartridge cannot be removed.
Insert a new staple cartridge into the staple case.
Push the staple cartridge in until it clicks into place.
Do not remove the seal from the cartridge before inserting the cartridge into the case.
Pull the seal that holds the staples straight out.
Push the staple case firmly back in.
Push the staple case in until it clicks into place.
Close the front cover.
Make a test print or copy in staple sort mode to verify that stapling takes place correctly.
Back to top