# F-CODE MEMORY BOX

This section explains how to store memory boxes for various types of F-code communication.

- [Add] key
  Adds a new memory box.
- List
  Lists the currently stored memory boxes. When you select a memory box, the edit/delete screen for the memory box appears.

Storing a memory box
When you tap the [Add New] key, the registration screen appears. Up to 100 F-code memory boxes can be stored for all functions (polling memory, confidential, and relay broadcast).
For information on the settings, see "Settings".
Editing and deleting a memory box
When you select a memory box from the list, the edit screen appears for the box.
For information on the settings, see "Settings".
Tap the [Delete] key to delete the memory box.
Settings

Item | Description
--- | ---
Items common to all types
Box Type | Select the type of box. Polling Memory: Store a memory box for F-code polling memory. The sub-address and passcode that you store in the memory box are necessary for the other machine to poll the machine (request transmission) using F-code communication. Confidential: Store a memory box for F-code confidential communication. In addition, store a "Print PIN" in the memory box to print faxes received by confidential reception. The sub-address and passcode that you program in the memory box are necessary for the other machine to send a fax to the machine by F-code confidential transmission. Relay Broadcast: Store a memory box for F-code relay broadcast transmission. Up to 30 destinations can be stored to forward the received data. The sub-address and passcode that you program in the memory box are necessary for the other machine to send a fax to the machine by F-code relay request transmission.
Memory Box Name | Enter a name (maximum of 18 characters) for the memory box.
Sub Address/Passcode | Enter a sub-address and passcode. A maximum of 20 digits can be entered for each sub-address and passcode. Separate a sub-address and passcode by a slash ("/").
Items displayed when storing a confidential memory box
Print PIN | Set a "Print PIN" for confidential reception. Enter a 4-digit number.
Items displayed when storing a relay broadcast memory box
Recipients | Select the end recipients of the relay broadcast. Select the recipients from the address book. Select the recipient from the address book: Selects an address from the address book. Destination Entry: An address that is not stored in the address book can be directly entered. Enter the address in the same way as when storing an address for a mode. Address Review: This displays a list of the selected recipients. Addresses can be deleted from this list if needed.

- When programming a new memory box, a sub-address that is already programmed for another box cannot be used. However, the same passcode can be used for more than one memory box.
- [] and [#] cannot be used in a sub-address.

- A passcode can be omitted.
- Do not forget the Print PIN. In the event that you forget the Print PIN or need to verify the Print PIN, contact your dealer or nearest authorised service representative.

Back to top