# SEND SETTING TO DESTINATION RUNNING IN MULTIPLE OPERATION MODES

## Overview

When you broadcast a document to the destination running in multiple operation modes such as Scanner mode, your setting is reflected in all modes, even if you have set the transmission on any mode screens. Note the following exceptions:

Send size | If an original larger than A4 (8-1/2" × 11") is scanned, it will automatically be reduced to A4R (8-1/2" × 11"R) before transmission.
Resolution (image) | Pages are sent using settings configured in each mode.
File format (file compression mode) | In "Setting mode (administrator)", select [System Settings] → [Image Send Settings] → [Scan Settings] → [Scan Settings], and the compression format selected by [Compression Mode at Broadcasting] is used.
Colour scanning | In scan mode, if the colour mode setting is [Full Colour], the original is sent in colour to scan destinations.
Original count | This is valid in the currently selected mode only.
Scan file size | In "Setting mode (administrator)", select [System Settings] → [Image Send Settings] → [Scan Settings] → [Scan Settings] → [Compression Mode at Broadcasting]. If the broadcast destination has the data size limit being set by [Maximum Size of E-mail Attachments (E-mail)] or [Maximum Size of Data Attachments (FTP/Network Folder)], the destinations having no such limit are also restricted.
Dropout colour | This mode is available for Scanner and Data entry. It is linked to a mode with an appropriate function.

Back to top