# DIRECTLY PRINTING A FILE IN A NETWORK FOLDER

## Overview

You can specify and print a file in a network folder from the touch panel of the machine. Even if the network folder is not registered, you can access the network folder by directly entering or referring to the path to the folder in the workgroup.
When you select a password-protected PDF file, you must enter the password in the job status screen.

- PRINTING AN ENCRYPTED PDF FILE

###### To register a network folder:

In "Setting mode (administrator)", select [Application Settings] → [Setting for Print from the MFP(SMB)]. Up to 20 network folders can be registered.

## Operation

### Printing a file in the network folder you have configured in the machine's settings

1. #### Tap the [HDD File retrieve] key

2. #### Tap the [Select File from Network Folder to Print] key on the action panel

3. #### Tap the [Open Registered Network Folder] key on the action panel and tap the network folder that you wish to access

   If a screen appears prompting you to enter a user name and password, check with your server administrator and enter the appropriate user name and password.

4. #### Tap the key of the file that you wish to print, and tap the [Choose Print Settings] key on the action panel

   - When printing multiple files, tap all the files you wish to print, and tap the [Print] key on the action panel.
   - The checkboxes of the selected files are selected.
   - The icon appears to the left of the keys of files that can be printed.
   - The icon is displayed to the left of keys of folders in the network folder. To display a folder or a file in a folder, tap this key.

   - A total of 100 keys of files and folders can be displayed.
   - Tap to move up one folder level.
   - To return to the network folder selection screen, tap .
   - Tap the [File or Folder Name] key to change the order of the files and folders displayed on the screen. Each time the key is tapped, the order changes between ascending and descending.

5. #### Select the print conditions

   - If you have selected multiple files in step 4, you can only select the number of prints.
   - If you have selected a file that includes print conditions (i.e., PCL, PS, or XPS files) in step 4, the settings will be applied.
   When the [Print Glossy] checkbox is selected, [Paper Area] is set to [Glossy Paper] (bypass tray) and [Resolution] is set to [600 dpi (High Quality)].

6. #### Tap the [Start] key

   Printing begins after the selected file is transferred.

### Entering the network folder path directly to print a file

1. #### Take steps until step 2 of "Printing a file in the network folder you have configured in the machine's settings"

2. #### Tap the [Direct Input of Folder Path] key on the action panel

3. #### Enter the path to the folder, user name and password

   Access the network folder.
   For the procedure for printing, see steps 4 to 6 of "Printing a file in the network folder you have configured in the machine's settings".

### Specifying the network folder path for each level to print a file

1. #### Tap the key of the workgroup that you wish to access in step 3 of "Printing a file in the network folder you have configured in the machine's settings"

2. #### Tap the key of the server or computer that you wish to access

   If a screen appears prompting you to enter a user name and password, check with your server administrator and enter the appropriate user name and password.

3. #### Tap the key of the network folder that you wish to access

   Access the network folder.
   For the procedure for printing, see steps 4 to 6 of "Printing a file in the network folder you have configured in the machine's settings".
   - Tap the icon and enter a keyword to search for a workgroup, server, or network folder. For how to enter text, see "NAMES AND FUNCTIONS OF SOFT KEYBOARD KEYS ".
   - Up to 100 workgroups, 100 servers, and 100 network folders are displayed.
   - Tap to move up one folder level.
   - To return to the workgroup selection screen, tap .

Back to top