# ADJUSTING THE SHARPNESS OF AN IMAGE (SHARPNESS)

## Overview

This function adjusts the sharpness to make a sharper or softer image.
Sharpness must be specified before scanning the original.

## Operation

1. #### Tap the [Others] key, and tap the [Sharpness] key

2. #### Tap or slide the slider to adjust the sharpness

   After the settings are completed, tap and the [Back] key in sequence.

   ###### To cancel the sharpness setting:

   Tap the [Off] key.

3. #### Place an original, and tap the [Preview] key

   Place the original in the automatic document feeder or on the document glass.
   - AUTOMATIC DOCUMENT FEEDER
   - DOCUMENT GLASS

   ###### To cancel all settings:

   Tap the [CA] key.

4. #### Tap the [Start] key to start copying

   ###### To make two or more sets of copies:

   Tap the copies display key to specify the number of copies.

Back to top