# QUICK SETTINGS

Select the minimum required settings for the machine connection to the network.
When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### IPv4 Settings

When using the machine on a TCP/IP (IPv4) network, use this setting to configure the IP address of the machine.

###### DHCP/BOOTP

Use this setting to have the IP address obtained automatically using DHCP (Dynamic Host Configuration Protocol)/BOOTP (Bootstrap Protocol). When this setting is enabled, it is not necessary to manually enter an IP address.
If the machine is used on a TCP/IP network, be sure to enable the "TCP/IP".
If DHCP/BOOTP is used, the IP address assigned to the machine may change automatically. If the IP address changes, printing will not be possible.

###### IPv4 Address

Enter the IP address of the machine.

###### Subnet Mask

Enter the IP subnet mask.

###### Default Gateway

Enter the default gateway address.

### IPv6 Settings

When using the machine on a TCP/IP (IPv6) network, use this setting to configure the IP address of the machine.

###### IPv6

Enable this setting.

###### DHCPv6

Use this setting to have the IP address obtained automatically using DHCP (Dynamic Host Configuration Protocol) v6. When this setting is enabled, it is not necessary to enter an IP address.

###### Manual Address/Prefix Length

Enter the IP address and the prefix length (0 to 128) of the machine.

###### Default Gateway

Enter the default gateway address.

- If the machine is used on a TCP/IP network, be sure to enable the "TCP/IP" below.
- In an IPv6 environment, the machine can use LPD or IPP protocol.

- If DHCPv6 is used, the IP address assigned to the machine may change automatically. If the IP address changes, printing will not be possible.

### Network Name Settings

###### Device Name

Enter a device name.

###### Domain Name

Enter the domain name.

### DNS Settings

###### Primary Server

Enter the IP address of primary DNS server.

###### Reply E-mail Address

Enter the IP address of secondary DNS server.

###### Domain Name

Enter the domain name where the selected DNS server exists.

### SMTP Settings

###### Primary Server

Enter the IP address or the host name of the primary SMTP server.

###### Reply E-mail Address

If data transmission has failed, the undelivered e-mail may be returned from the server. Enter an e-mail address (a single address only) to receive such undelivered mails. Usually, enter the e-mail address of the system administrator.

###### Enable SSL

If is selected, the SMTP-over-TLS encryption communication can be used by STARTTLS command.
This requires the server to support the STARTTLS command.
To allow SSL communication, set the "Port Number" to the same port number as the normal SMTP.

###### SMTP Authentication

If is set, the SMTP server authentication is carried out.

###### User Name

Enter the user name.

###### Password

To change the password, set the [Change Password] checkbox to and enter the new password.

###### Connection Test

Tap the [Execute] button to test the connection to the SMTP server.

### LDAP Settings

###### Name

Enter the address book name.

###### Default Address Setting

Enters the search defaults to search for a specific area of the LDAP directory information tree.
Example: o = ABC, ou = NY, cn = Everyone
Entries must be separated by semicolons or commas.

###### LDAP Server

Enter the IP address or host name of the LDAP server.

###### User Name

Enter the account name for LDAP setting.

###### Password

To change the password, set the [Change Password] checkbox to and enter the new password.

###### Authentication

Select the authentication server from the drop-down list.

###### KDC Server

Enter the IP address or host name of the Kerberos authentication server.

###### Realm

Enter the Kerberos realm.

###### Enable SSL

If is set, the SSL encryption communication is enabled.

###### Connection Test

Tap the [Execute] button to test the connection to the LDAP server.

### Public Folder / NAS Setting

Set each option to [Prohibited] if the storage is not used.
Back to top