# SENDING BOTH SIDES OF A CARD AS A SINGLE PAGE (CARD SHOT)

## Overview

Send the front and reverse sides of a card as a single page, without the need to send each side separately.

Place the original on the document glass.

- If the scan size is larger than the send size, it will result in a sending failure.
- The ratio cannot be specified and "Rotation Sending Setting" cannot be selected.

## Operation

1. #### Place a card face down on the document glass

   - DOCUMENT GLASS

2. #### Specify the destination

   - SPECIFYING A DESTINATION FROM THE ADDRESS BOOK
   - SPECIFYING A DESTINATION USING THE SEARCH NUMBER
   - ENTER A DESTINATION MANUALLY
   - SPECIFYING A DESTINATION FROM THE GLOBAL ADDRESS BOOK
   - SPECIFYING A DESTINATION FROM TRANSMISSION LOG

3. #### Tap the [Others] key, and tap the [Card Shot] key

4. #### Tap the [On] key, and specify the original size as required

   Tap the areas displaying width and height sizes of the original respectively, and enter the sizes using the numeric keys.
   Or tap to enter the size.
   After the settings are completed, tap and [Back] keys in sequence.

   - If you check the [Fit to Send Size] box to , the original is enlarged or reduced by the ratio appropriate to the original size.
   - After selecting Card Shot, tap the [Original] key on the initial screen to change the original scan size or the send size. In this case, the screen of this step appears when you tap the scan size key. For the procedure for setting the send size, see "SPECIFYING THE SEND SIZE OF THE IMAGE".
   - To cancel the specified size settings, tap the [Size Reset] key.

   ###### To cancel the Card Shot settings:

   Tap the [Off] key.

5. #### Tap the [Start] key to scan the front side

   Tap the [Preview] key, and you can preview the output image before sending it.
   For more information, see "CHECKING THE OUTPUT IMAGE BEFORE TRANSMISSION". However, settings for this function cannot be changed in the preview screen.

6. #### Place a card face up on the document glass, and tap the [Start] key to scan the reverse side

   - Before scanning the back of the card, tap the [Function Rev.] key on the touch panel to change the exposure.
   - After checking the output by [Preview] key, tap the [Additional Scan] key to scan the next original. Tap the [Start] key to start sending an image. Now, Step 7 is not required.

7. #### Tap the [Read-End] key

   A beep will sound to indicate that transmission has ended.
   If you will continue by scanning the front of the card, you can tap the [Function Rev.] key to change the exposure, resolution, scan size, and send size.

Back to top