# SPECIFYING THE SEND SIZE OF THE IMAGE

## Overview

Tap this key to specify the send size as a paper size.
For example, if the scan size is A4 (8-1/2" × 11") and the send size is 5-1/2" × 8-1/2" (B5), the image will be reduced before transmission.

The send size cannot be specified when [Long Size] is selected for the scan size, or when the scan size is specified by numeric values.

## Operation

1. #### Tap the [Original] key

2. #### Tap the "Send Size" key

3. #### Tap the appropriate paper size key

   After the settings are completed, tap .

   Depending on the paper size specified for the "Scan Size", it may not be possible to select some sizes for the "Send Size".

4. #### Tap the "Image Orientation" key with the same orientation as the original image

   If this setting is not correct, a suitable image may not be transmitted.
   After the settings are completed, tap .

   The ratio used for reduction or enlargement of the original will appear between the "Scan Size" and the "Send Size".
   To configure the default setting of image orientation, select [System Settings] in "Setting mode (administretor)" → [Image Send Settings] → [Operation Settings] → [Default Settings] → [Image Orientation].

Back to top