# INSERTING INSERTION SHEETS IN BETWEEN TRANSPARENCY FILMS (TRANSPARENCY INSERTS)

## Overview

When copying on transparency film, the sheets may stick together due to static electricity.
The transparency inserts function can be used to insert a sheet of paper between each sheet of transparency film, making the sheets easy to handle.
It is also possible to copy on insertion sheets.

- When performing 2-sided copying, only "2-Side to 1-Side" mode can be used.
- Transparency film can be loaded in the bypass tray, tray 4 and large capacity trays.

The number of copies cannot be selected in this mode.

## Operation

1. #### Load transparency film in the bypass tray, tray 4 or large capacity trays

   When using the bypass tray, place the paper with the print side up.
   - BYPASS TRAY
   - TRAY 3/4
   - LARGE CAPACITY TRAYS

2. #### Set the tray

   - SETTING THE PAPER TRAY

3. #### Place an original, and tap the [Preview] key

   Place the original in the automatic document feeder or on the document glass.
   - AUTOMATIC DOCUMENT FEEDER
   - DOCUMENT GLASS

4. #### Tap the [Others] key, and then tap the [Transparency Inserts] key

5. #### Tap the [On] key

   When making a copy on insertion sheets, tap the [Also Make Copy on Inserts] checkbox to set to .
   After the settings are completed, tap and the [Back] key in sequence.

   ###### To cancel the transparency inserts setting:

   Tap the [Off] key.

6. #### Check the preview image in the preview screen

   ###### To cancel all settings:

   Tap the [CA] key.

7. #### Tap the [Start] key to start copying

Back to top