# PRINT PORT SETTINGS

## "LPD" Tab

Enter a profile expiring date.
When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### LPD Settings

###### LPD

Set this option to use LPD.

###### Timeout

Enter a timeout. The default setting is 90 seconds.

###### Use Banner

Set this option to use the banner. The default setting is [Disable].

## "RAW" Tab

Use this tab to configure Raw print.
When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### Raw Print Settings

###### Raw Print

Set this option to use RAW printing. The default setting is [Enable].

###### Port Number

Enter a port number. The default setting is port 9100.

###### Timeout

Enter a timeout. The default setting is 90 seconds.

###### Use Bidirectional

To use bidirectional communication, set to .

## "WSD" Tab

Use this tab to configure WSD print.
When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### WSD Settings

###### WSD Print

Set this option to use WSD printing.

###### Use Multicast Discovery

Set this option to use multicast discovery.
Back to top