# SPECIFYING A DIFFERENT RATIO FOR X AND Y

## Overview

This section explains how to individually specify the horizontal and vertical copy ratios.
There are two methods to determine the ratio: specifying the range from 25% to 400% on a 1% basis for both the horizontal and vertical copy ratios and specifying the original image size and output image size.
When 50% is selected for the horizontal ratio and 70% is selected for the vertical ratio

When the automatic document feeder is used, the vertical and horizontal ratio selection ranges are both between 25% to 200%.

###### To cancel the XY zoom setting:

Tap the [Zoom] tab or the [CA] key on the ratio setting screen.

## Operation

### Using the preset ratio key

1. #### Tap the [Copy Ratio] key, and then tap the [XY Zoom] tab

2. #### Tap the [X] key, and set the X (horizontal) ratio

   To quickly set the ratio, first specify a value close to the desired one, then adjust it with .
   Tap each area of the X (horizontal) and Y (vertical) directions, and enter the sizes using the numeric keys.

3. #### Tap the [Y] key, and set the Y (vertical) ratio in the same way as the [X] key

   After the settings are completed, tap .
   Check that a paper size suitable for the ratio is selected.

### Specifying the image dimensions

1. #### Tap the [Copy Ratio] key, and then tap the [XY Zoom] tab

2. #### Tap the [by Size] key

3. #### Specify the original image size and output size

   Tap the area of image size and output size, and enter the sizes using the numeric keys.
   Check that a paper size suitable for the ratio is selected.
   After the settings are completed, tap .

   - ###### If you have entered an incorrect size:

     Tap the [C] key, and then enter the correct size.

   - ###### To cancel all settings:

     Tap the [CA] key.

Back to top