# EXTERIOR

This section describes the names and functions of the respective parts on the exterior of the machine.
Tap the name to make its details pop up.

The indicators of the operation panel may differ depending on the country and region.
×
Automatic document feeder
This automatically feeds and scans multiple originals. Both sides of 2-sided originals can be automatically scanned at one time.
-AUTOMATIC DOCUMENT FEEDER
×
Front cover (upper)
Open this cover to replace the toner cartridge or to remove misfed paper in the paper pass unit.
×
Status indicator*
The status of the machine is indicated.
-STATUS INDICATORS
×
Front cover (lower)
Open this cover to switch the main power switch to "On" or "Off" or to clean the main charger of the photoconductive drum.
-TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE
- TONER CARTRIDGE
- Cleaning the laser unit
×
Output tray (centre tray)*
Printed paper is output into this tray.
×
Operation panel
This panel hosts the [POWER] button, [Power Save] button/indicator and touch panel. Use the touch panel to operate each of these functions.
-OPERATION PANEL
×
Right tray*
As required, paper can be output into the right tray.
×
Finisher*
This staples and outputs paper.
×
Saddle finisher*
This staples and folds paper.
×
Curl correction unit*
This corrects curls in printed paper.
×
Punch module*
This punches holes in paper.
×
USB port (A type)
This is used to connect a USB device such as a USB memory device to the machine.
For the USB cable, use a shielded cable.
Supports USB 2.0 (Hi-Speed).
×
Keyboard
Use this as a substitute for the soft keyboard displayed on the touch panel. When not being used, it can be stored under the operation panel.
-NAMES AND FUNCTIONS OF SOFT KEYBOARD KEYS
×
Tray 1
Store paper in this tray. Up to 1,200 sheets can be stored.
-TRAY 1/2
×
Tray 2
Store paper in this tray. Up to 800 sheets can be stored.
-TRAY 1/2
×
Tray 3
Store paper in this tray. Up to 500 sheets can be stored.
-TRAY 3/4
×
Tray 4
Store paper in this tray. Up to 500 sheets can be stored.
-TRAY 3/4
×
Tray 5 (MX-LC12)*
Store paper in this tray. Up to 3,500 sheets can be stored.
-LARGE CAPACITY TRAY
×
Tray 5 (MX-LCX3 N)*
Store paper in this tray. Up to 3,000 sheets can be stored.
-LARGE CAPACITY TRAY
×
Bypass tray*
Use this tray to feed paper manually.
When loading paper larger than A4R or 8-1/2" × 11"R, pull out the extension guide.
-BYPASS-TRAY
×
Trimming module*
This trims the excess of saddle-stitched output.

×
Large capacity trays*
Store paper in this tray. Up to 2,500 sheets can be stored in each tray.
-LARGE CAPACITY TRAYS
×
Bypass tray*
Use this tray to feed paper manually.
When loading paper larger than A4R or 8-1/2" × 11"R, pull out the extension guide.
×
Inserter*
Covers and insertion sheets to be inserted into printed sheets can be loaded.
Using the manual finishing function, you can directly feed paper into the finisher or saddle finisher to staple, punch or fold the paper.
×
Folding unit*
This folds and outputs paper.
×
Paper cart*
This is a cart that is installed in the high capacity stacker. It is useful when you carry a large number of output sheets.
×
High capacity stacker*
This unit is useful when you output a large number of copies. A maximum of 5,000 sheets of paper can be output.
You can also connect two units.
-HIGH CAPACITY STACKER
* Optional. Back to top