# PRINTING WITHOUT TOP AND BOTTOM MARGINS

## Overview

This function enables printing without top and bottom margins. By combining this function with the saddle stitch printing and trimming functions, a booklet or pamphlet without margins can be created.
This function can only be used for A3/11" x 17" and A4/8-1/2" x 11" sizes. To use this function effectively, create document data in the application that is 2 mm longer than the top and bottom of the paper, and 2 mm shorter in the direction of feeding. When using any other document sizes, use the Fit to Page function.

- This function is available in a Windows environment.
- Printer driver PCL6 or PS can use this function.

## Operation

### Windows

### Saddle stitch printing and 2-position stapling

1. #### Click the [Paper] tab and set the [Edge-to-Edge Printing] checkbox to set to

2. #### Click the [Main] tab and select [Pamphlet Style]

3. #### Select [2 Staples]

4. #### Configure Trimming settings

   (1) Click the [Trimming...] button
   (2) Set the [Trimming Width] checkbox to set to
   (3) Specify "5.0 mm (0.200 inches)"

### Fold stapling

1. #### Click the [Paper] tab and set the [Edge-to-Edge Printing] checkbox to set to

2. #### Click the [Special Modes] tab, click the [Fold] button and then select [Mult-Sheet Fold - Staple]

3. #### Click the [Main] tab and configure Trimming settings

   (1) Click the [Trimming...] button
   (2) Set the [Trimming Width] checkbox to set to
   (3) Specify "5.0 mm (0.200 inches)"

### Single Sheet

1. #### Click the [Paper] tab and set the [Edge-to-Edge Printing] checkbox to set to

2. #### Click the [Main] tab and select [1-Sided], [2-Sided(Book)] or [2-Sided(Tablet)]

Check the actual print result. If margins appear, change the following settings.

- "Trimming Width" in the Trimming Settings dialog
- "Zoom Settings" in the [Paper] tab
- "Print Position" in the Compatibility dialog

Back to top