# RETRIEVING STORED COPY SETTINGS (CALL PROGRAM)

## Overview

This function collectively stores various settings as one program. If you store a program, you can easily retrieve and use it.
For example, suppose A3 (11" × 17") size CAD drawings are copied once a month for archive purposes using the following settings:

- The A3 (11" × 17") size CAD drawings are reduced to A4 (8-1/2" × 11") size.
- To reduce paper use by half, 2-sided copying is used.
- Margin shift is used to allow a margin to punch holes for filing.

When a job program is not stored | When a job program is stored
--- | ---
Sets A3 (11" × 17") to A4 (8-1/2" × 11") reduction Changes the exposure setting Sets 2-sided copying Sets margins Sets punch hole settings Tap the [Colour Start] key or the [B/W Start] key | Selects copy settings Tap the [Colour Start] key or the [B/W Start] key
This method requires multiple settings and takes time. Also, it may cause a setting error. | This method requires no multiple settings and takes no time. Also, you can make a copy with no setting errors.

- Up to 48 programs can be stored.
- Program settings remains registered even when the main power has been turned off.
- To store a program
  Tap the [Program Registration] key that appears on the action panel when you operate any mode screens.
  - STORING A PROGRAM

## Operation

1. #### Tap the [Call Program] key on the action panel

   If you tap the [Add to Favourites] or [Register for Home] key on the action panel, you can register a program shortcut key.

2. #### Tap the key of the program you want to retrieve

   The stored settings of the program are applied.

Back to top