# OUTPUT SETTINGS

## Overview

Configure the output settings for copies using Sort, Group, Offset, Staple, Punch, or Fold. Also specify the output destination of copies.

### Output Tray

Specify the destination to output copies.
Select the output tray from [Offset Tray] and [Right Tray]. If a finisher (100-sheet stapling) or saddle finisher (100-sheet stapling) is installed, you can select [Offset Tray], [Middle Tray] or [Right Tray].
If a high capacity stacker is installed, you can select [Top Tray] or [Stacker Tray].
If a finisher or saddle finisher is not installed, you can select the [Centre Tray] or [Right Tray] key.

- CHANGING OUTPUT DESTINATION

### Offset

This function outputs copies while shifting them set by set. Setting the checkbox to enables the offset function, and setting it to disables the function.
This function is available only when the finisher or saddle finisher is installed.
Selecting the staple function clears the Offset checkmark automatically.

### Separator Page

The function inserts separator pages for every specified number copies or for every job before they are output.

### Sort/Group

Select the sorting method when copying the scanned original.
"Sort" sorts the scanned original on a set basis, and outputs them. "Group" sorts the scanned original on a page basis, and outputs them.

- CHANGING THE METHOD TO ORGANIZING OUTPUT

### Staple

Each set of copies can be stapled, or the sheets can be folded at the centre and stapled.

- The staple function is available only when the finisher or saddle finisher is installed.
- The saddle stitch function is available only when the saddle finisher is installed.

- STAPLING EACH SET OF SORTED COPIES
- SADDLE STITCHING FOR SORTED COPIES

### Fold

Copies can be folded and output.
The fold function is available only when the saddle finisher or folding unit is installed.

- FOLDING OUTPUT PAPER

### Punch

This function punches copies and outputs them.
The punch function is available only when the punch module is installed.

- PUNCHING COPIES

Back to top