# AUTO POWER SHUT-OFF TIMER

## Overview

This mode turns off the power to the operation panel and the fusing unit, and makes the machine wait in the lowest power consumption state.
Auto Power Shut-Off Timer will activate when the set duration of time elapses in waiting status without executing a job.
Compared to preheat mode, the power-saving rate is considerably higher but the wakeup time is longer.
The [Power Save] button blinks when the machine is in Auto Power Shut-Off Timer.
Auto Power Shut-Off Timer is also activated by holding down the [Power Save] button while the [Power Save] button is not lit.
This mode is cleared when print data is being received is being output or when the [Power Save] button is pressed while it is blinking.

This function is not available in some countries and regions.
A message appears 15 seconds before Auto Power Shut-Off Mode is entered. To close the message and continue normal operation, tap the [Continue] button.
The message appears again 15 seconds before the end of the extension of normal operation time.
If no action is taken within 15 seconds after the message appears, the machine enters auto power shutoff mode.

###### To set display of the message:

Set in [Energy Save] → [Power Management Setting] → [Display message for delay of entry into Preheat Mode / Auto Power Shutoff] in "Setting mode (administrators) ".
Back to top