# DIRECTLY PRINTING A FILE IN AN FTP SERVER

## Overview

If you register an FTP server, you can specify a file in the FTP server from the touch panel on the machine. This saves you the trouble of downloading the file and printing it from the computer.
When you select a password-protected PDF file, you must enter the password in the job management screen.

- PRINTING AN ENCRYPTED PDF FILE

###### To register an FTP Server:

In "Setting mode (administrator)", select [Application Settings] → [Setting for Print from the MFP(FTP)]. Up to 20 FTP servers can be registered.

## Operation

1. #### Tap the [HDD File retrieve] key

2. #### Tap the [Select File from FTP to Print] key on the action panel

3. #### Tap the FTP server you wish to access

   Some server may require you to enter the user name and password.

4. #### Tap the file that you wish to print, and tap the [Choose Print Settings] key on the action panel

   - When printing multiple files, tap all the files you wish to print, and tap the [Print] key on the action panel.
   - The checkboxes of the selected files are selected.
   - The icon appears to the left of the keys of files that can be printed.
   - The icon is displayed to the left of the keys of folders in the FTP server. To display a folder or a file in a folder, tap this key.

   - A total of 100 keys of files and folders can be displayed.
   - Tap to move up one folder level.
   - When you move down a folder level by tapping a folder key, appears.
     Tap this key to return to the file or folder name selection screen.
   - Tap the [File or Folder Name] key to change the order of the files and folders displayed on the screen. Each time the key is tapped, the order changes between ascending and descending.

5. #### Select the print conditions

   - If you have selected multiple files in step 4, you can only select the number of prints.
   - If you have selected a file that includes print conditions (i.e., PCL, PS, or XPS files) in step 4, the settings will be applied.
   When the [Print Glossy] checkbox is selected, [Paper Area] is set to [Glossy Paper] (bypass tray) and [Resolution] is set to [600 dpi (High Quality)].

6. #### Tap the [Start] key

   Printing begins after the selected file is downloaded.

Back to top