# READING THE JOB LIST

The meaning of each job icon and message displayed in "Status" is as follows:

- Icons indicating the job type
- Messages displayed in "Status"

Icons indicating the job type

| Print job (RGB/CMYK) |  | Copy job
| Scan to E-mail job |  | Scan to FTP job
| Scan to Network Folder job |  | Scan to Desktop job
| Fax transmission job |  | Fax reception job
| PC-Fax transmission job |  | Internet fax transmission job (Including Direct SMTP)
| PC-I-Fax transmission job |  | Scan to HDD file print job
| Internet fax reception job (Including Direct SMTP) |  | Broadcast job* Inbound routing job
| Tandem copy/print job |  | Reprinting of multiple files (as grouped into a single file)
| OSA scan job |

* This appears in a multi-mode broadcast job.

Messages displayed in "Status"
Job in progress

Display | Status
--- | ---
"Printing" | Print job in progress
"Copying" | Copy job in progress
"Connecting" | Connecting
"Sending" | Sending
"Receiving" | Receiving
"Tel" | Speaking with the other party using an extension telephone
"Stopped" | The job has been stopped.
"FAST communications in progress" | FAST communications in progress
"Toner empty" | Toner Empty
"Paper empty" | Paper Empty
"Paper jam" | Paper jam
"Waiting" | Waiting
"Warming up" | Warming up
"Limit" | Having reached the account limit
"Error" | An error occurred while the job was being executed.

Reserved job

Display | Status
--- | ---
"Waiting" | The job is waiting to be executed.
"Retry Mode" | The job is being retried due to a communication error or other problem.
"Waiting for confirmation of the transmission" | Waiting for confirmation of Internet fax transmission
A day and time is displayed | Timer transmission job (the specified time is displayed)

Completed job

Display | Status
--- | ---
"OK" | Normal termination
"Send OK" | Transmission was completed.
[In Memory] | Reception completed but the fax has not been printed. The received data (each page) has not been printed or forwarded. (The received data has not been deleted.)
"Received" | Printed received fax data. The fax has been received. The received data (each file) was stored.
"Forward OK" | The received data/received data (each file) has been forwarded.
"FAST communications in progress" | FAST communications in progress
"Stopped" | The job was stopped.
"Delete" | Deleted received data in the image check screen.
"Number of successful transmission destinations/Total destinations OK" | Completion of a broadcast transmission, serial polling, or inbound routing operation. If transmission to 3 destinations was successful out of a total of 5, "003/005 OK" will appear.
"No response" | An error occurred because there was no response from the destination.
"Busy" | An error occurred because the other party was busy.
"OK REPORT" | A "Successful reception" reply received
"NG REPORT" | A "Delivery error" reply received
"NO REPORT" | Delivery Confirmation Receive Timeout
"E-mail received" | E-mail other than Internet fax received
"Rejected" | A fax was sent from a party that has been blocked by the anti junk fax function.
"NGxxxxxx" | Transmission/reception was not successful because a communication error occurred (a 6-digit error code appears in xxxxxx.)
"Error" | An error occurred while the job was being executed.

Back to top