# THE IMAGE IS UPSIDE DOWN

If you are unable to solve a problem using the solutions in this manual, press the [Power] button and then turn the main power switch to the "" position. Wait at least 10 seconds and then turn the main power switch to the "" position. After the main power indicator colour changes to green, press the [POWER] button.
When the background colour of the job status display at the upper right corner of the touch panel is not grey, do not switch off the main power switch or unplug the power plug. This may damage the hard drive or cause the data being stored or received to be lost.

Point to check | Solution
--- | ---
Are you using a type of paper (tab paper, punch paper, etc.) that can only be loaded in a fixed orientation? | Rotate the image 180 degrees before printing. When the image size and paper size are the same but the orientations are different, the orientation of the image is automatically rotated to match the paper. However, when the paper can only be loaded in a fixed orientation, the image may be printed upside down. In this event, rotate the image 180 degrees before printing. Windows: The setting is selected in the [Main] tab of the printer driver. Macintosh (OS X 10.4 to 10.5): The setting is selected using the [Page Setup] menu. (Landscape orientation only)
Is the correct binding position selected for 2-sided printing? | Be sure to set the appropriate binding position. When 2-sided printing is performed, every other page is printed upside down when tablet binding is selected for the binding position. Windows: The setting is selected in the [Main] tab of the printer driver. Macintosh: The setting is selected in the [Layout] menu of the print window.

Back to top