# METADATA SETTING

If the Application Integration Kit is installed, you can control the metadata to be used in other applications.
The stored metadata is displayed on the metadata settings page. You can add a metadata, and edit or delete an existing metadata.

- [Add] key
  Adds a new metadata set.
- List
  Lists the currently stored metadata sets.

Metadata Delivery
Enables or disables the metadata delivery function.
Storing Metadata Sets
When you tap the [Add] key, the registration screen appears. Up to 10 items can be stored.
For information on the settings, see "Settings".
Edit or Delete Metadata Set
When you tap a title on the list, the edit screen appears for that metadata set.
Tap the [Delete] key to delete the metadata set.
Settings

Item | Description
--- | ---
Metadata Set Name | Enter a metadata name.
Metadata Delivery Destination | Select a destination where you wish to send the image and metadata.
Allow Custom Filenames | Enable or disable to edit the name of image file and XML file to be sent by the metadata send job.
Address Type Allowing Metadata Entry | Set the destination information to be used for metadata transmission.
Name | Enter a metadata name to be displayed on the touch panel.
XML Tag Name | Enter an XML tag name to be contained in the metadata set.
Entry Type | Direct entry: Allows direct entry of each metadata from the soft keyboard or the numeric keypad. Metadata list: Allows a selection of metadata from the previously entered data list. You must enter optional values for metadata selection in the input area. Entries must be separated by semicolons or commas. Each option can be comprised of up to 70 characters. Initial entry by default: Uses a default value as the first value of the entered metadata list.
Expand Metadata Automatically | When the machine generates metadata automatically, the "metadataSetName", "userLoginId" (if user authentication is used), "pageSize", and "imageMode" are added to the metadata.
To Be Used as Default | The current metadata set is used as the default.

Back to top