# EXTERNAL ACCOUNTING APPLICATION SETTINGS

An external account application can be added and controlled.
Set the server name where you have installed the external accounting application.

Item | Description
--- | ---
External Account Control | Enable the totalling function by the external accounting application. If enabled, always enter the application name or Web service address.
Set Authentication Server (Server 1) | If the server is set, the external authentication mode is selected. Any access to the MFP is controlled by the application that you set on this page. If set, always enter the application name, application UI address, or Web service address of server 1. If not set, the external totalling mode is selected.
Enable Image Job Log | This item is displayed when you enter a product key of the "Sharp Document Recorder."
Server 1-4 | Select a server to enable it.
Application Name | Enter an application name.
Application UI Address | Enter the URL of the login screen to be accessed first when the machine is turned on.
Web Service Address | Enter the URL of the server or computer which sends commands and events by XML/SOAP protocol.
Timeout | Enter a timeout. The default setting is 20 seconds.
Home Directory Path | Enter a maximum of 64 half-width characters for the home directory search text.
User Name | Enter a maximum of 127 full-width/half-width characters for the user name for home directory path authentication.
Password | Enter a maximum of 255 numeric digits for the password for home directory path authentication.

Back to top