# MANUAL RECEPTION/POLLING RECEPTION ARE NOT POSSIBLE

If you are unable to solve a problem using the solutions in this manual, press the [Power] button and then turn the main power switch to the ""position. Wait at least 10 seconds and then turn the main power switch to the ""position. After the main power indicator colour changes to green, press the [POWER] button.
When the background colour of the job status display at the upper right corner of the touch panel is not grey, do not switch off the main power switch or unplug the power plug. This may damage the hard drive or cause the data being stored or received to be lost.

Point to check | Solution
--- | ---
Is little free memory remaining? | If any of the following applies, print or delete received faxes to increase available memory space for receiving faxes. The memory contains data that has been received with the received image check setting enabled. The memory contains data that has been received with confidential reception or that is protected by a password. A fax is stored in the memory box.

Back to top