# SETTING FOR PRINT FROM THE MFP (FTP)

From the operator panel of machine, you can access the FTP server and select server data for printing.

- [Add] key
  Adds a new FTP server.
- List
  Lists the currently stored FTP servers.

Store FTP Server
When you tap the [Add] key, the registration screen appears. Up to 20 items can be stored.
For information on the settings, see "Settings".
Edit or Delete FTP Server
When you tap a title on the list, the edit screen appears for that FTP server.
Tap the [Delete] key to delete the FTP server.
Settings

Item | Description
--- | ---
Name | Enter a name to be displayed on the machine operator panel.
FTP Server | Enter the IP address or host name of the FTP server.
Directory | Enter the destination directory of the FTP file server.
Enable User Authentication | Enables user authentication. The user name and password are required to enter.
User Name | Enter the login user name for logging in the FTP file server.
Password | Enter the password required for logging in the FTP file server. To change the password select [Change Password] , and enter the new password in the text box.
Enable SSL | Enables the SSL encryption communication.

Back to top