# PRINTING IS NOT POSSIBLE OR STOPS DURING A JOB

Point to check | Solution
--- | ---
Is a tray out of paper? | Add paper as instructed by the message in the touch panel.
Is the machine out of toner? | Replace the toner cartridge. When toner runs low, a message will appear to inform you that the toner cartridge must be replaced. For more information on replacing the toner cartridge, see "REPLACING THE TONER CARTRIDGE".
Has a paper misfeed occurred? | Remove the misfeed as instructed by the message in the touch panel. - "REMOVING MISFEEDS" in "TROUBLESHOOTING"
Is the output tray full? | Remove the output from the tray and resume printing. When the output tray becomes full, a detector activates and stops printing.
Is the toner collection container full? | Replace the toner collection container as instructed by the message in the touch panel. - "REPLACING THE TONER COLLECTION CONTAINER"
Are restrictions placed on the trays that can be used in each mode (copy, print, fax, Internet fax, and document filing)? | Check the settings in [Paper Tray Settings] and see if checkmarks appear in the checkboxes of each mode ([Feeding Approved Job]). Functions without a checkmark cannot be used for printing using that tray. "Setting mode" → [Paper Tray Settings] → [Tray Registration] → [Feeding Approved Job]

Back to top