# 2-SIDED COPYING DOES NOT TAKE PLACE

If you are unable to solve a problem using the solutions in this manual, press the [Power] button and then turn the main power switch to the ""position. Wait at least 10 seconds and then turn the main power switch to the ""position. After the main power indicator colour changes to green, press the [POWER] button.
When the background colour of the job status display at the upper right corner of the touch panel is not grey, do not switch off the main power switch or unplug the power plug. This may damage the hard drive or cause the data being stored or received to be lost.

Point to check | Solution
--- | ---
Does the paper type setting of the selected tray specify a type of paper that cannot be used for 2-sided copying? | Check "Tray Settings" in the setting mode. If the [Disable Duplex] checkbox is selected, 2-sided copying using that tray will not be possible. Change the paper type setting to a type that can be used for 2-sided printing. Set [System Settings] → [Paper Tray Settings] → [Tray Settings] → [Disable Duplex] to in "Setting mode".
Are you using a special size or type of paper? | For the paper types and sizes that can be used for two-sided copying, see "SPECIFICATIONS" in Quick Start Guide.
Are you copying using settings that do not allow 2-sided copying? | 2-Sided Copy can generally be combined with other modes as required, however, some combinations are not possible. If a prohibited combination is selected, a message will appear in the touch panel.
Have functions been disabled by the administrator? | Some functions may have been disabled in the setting mode. Check with your administrator. When user authentication is enabled, the functions that you can use may be restricted in your user settings. Check with your administrator.

Back to top