# SCANNING A THIN ORIGINAL(SLOW SCAN MODE)

## Overview

Use this function when you wish to scan thin originals using the automatic document feeder. This function helps prevent thin originals from misfeeding.
When slow scan mode is selected, 2-sided scanning is not possible.

## Operation

Place the original in the document feeder tray of the automatic document feeder.
Adjust the original guides slowly.

- AUTOMATIC DOCUMENT FEEDER

If the originals are inserted with too much force, they may crumple and misfeed.
Specify the destination.

- RETRIEVING A DESTINATION FROM AN ADDRESS BOOK
- VIEWING A LIST OF THE SELECTED DESTINATIONS
- USING A SEARCH NUMBER TO RETRIEVE A DESTINATION
- ENTERING AN ADDRESS MANUALLY
- SPECIFYING A NETWORK FOLDER
- RETRIEVING A DESTINATION FROM A GLOBAL ADDRESS BOOK
- USING A TRANSMISSION LOG TO RESEND

Touch the [Others] key, and tap the [Slow Scan Mode] key.
A checkmark appears on the icon.
To cancel the Slow Scan Mode setting:
Tap the [Slow Scan Mode] key to clear the checkmark.
After the settings are completed, tap the [Back] key.
Tap the [Start] key to start scanning of the original.
Tap the [Preview] key to check the preview of an image before sending a fax. For more information, see "CHECKING THE IMAGE TO BE TRANSMITTED". However, settings for this function cannot be changed in the preview screen.
A beep will sound to indicate that scanning and transmission have ended.
Back to top