# INBOUND ROUTING (HDD STORAGE) SETTINGS

Configure settings for saving received faxes to the hard disk.

Item | Description
--- | ---
Auto save of received faxes to HDD | Set whether received faxes are saved to the hard disk.
Set which faxes are saved | Select which received faxes are saved. Select from lines 1 to 3 and Internet Fax.
Specify the folder | Specify the folder in which received faxes are saved. Enter a folder name no longer than 32 full-width/half-width characters.
Enable/disable saving to folders by date | Configure settings to have date folders created and received faxes saved to the folders by date.
Received fax print settings | Configure print settings for received faxes. Save and print: Save received faxes to hard disk, and also print. Only print when save error occurs: Print received fax when save fails. Save in inbound routing error box when save fails: When save fails, save the fax in the inbound routing error box.
File format | Select the file format for inbound routing.
Preset characters | Set the characters added to the file name when a file is saved. When "Character 1" and "Character 2" are set in "File Naming No. 1 to No. 7", the set characters are added to the file name. Enter up to 64 full-width/half-width characters.
File Naming No.1 to No.7 | Set the information included in the file name when saving a file.
Reception notification settings | Set whether notification is sent by e-mail when a fax is received.
Notification address | Shows the address to which the notification is sent.
Direct Entry | Enter the notification address. Enter a maximum of 1500 half-width characters for the address.
Global Address Search | Select the address from the global addresses.
Add to list | An address directly entered or found by global address search is saved as the notification address.

Back to top