# DIRECTLY PRINTING A FILE ON AN FTP SERVER

## Overview

When an FTP server is configured, you can directly select and print files on the FTP server from the touch panel of the machine. This function eliminates the need for downloading the files from the FTP server to your PC and sending print jobs from the PC to the machine.
To configure an FTP server:
In "Setting mode", select [Application Settings] → [Setting for Print from the MFP(FTP)], and configure an FTP server. (Administrator rights are required.) Up to 20 FTP servers can be configured.
When you select a PDF file that has a password, you must enter the password in the job status screen to begin printing.

- PRINTING AN ENCRYPTED PDF FILE

## Operation

Tap the [Document Filing] key.
Tap the [Select File from FTP to Print] key on the action panel.
Tap the key of the FTP server that you wish to access.
Tap the key of the file that you wish to print, and tap the [Choose Print Settings] key on the action panel.

- When printing multiple files, tap the keys of the files you wish to print, and tap the [Print] key on the action panel.
- The icon appears to the left of keys of files that can be printed.
- The icon is displayed to the left of keys of folders on the FTP server. To display a folder or a file in a folder, tap this key.

- A total of 100 keys of files and folders can be displayed.
- Tap to move up one folder level.
- When you move down a folder level by tapping a folder key, appears.
  Tap this key to return to the file or folder name selection screen.
- Tap the [File or Folder Name] key to change the order of the files and folders displayed on the screen. Each time the key is tapped, the order changes between ascending and descending.

Select the print conditions.

- If you have selected multiple files in step 4, you can select only the number of prints.
- If you have selected a file that includes print conditions (i.e., PCL, PS, or XPS files) in step 4, the settings will be applied.

When the [Print on Glossy Paper] checkbox is selected, [Paper Select] is set to [Glossy Paper] (bypass tray) and [Output Resolution] is set to [600 dpi (High Quality)].
Tap the [Start] key.
Printing begins after the selected file is downloaded.
Back to top