# CARD AREA SETTING

The data check during card reading can be set.

###### List of Set Up Items

Item | Description
--- | ---
Import from Configuration file | When you enter the configuration file name and tap the [Execute] key, the card area settings are read from the configuration file. If you tap the [Clear] key, all files that match the current search conditions are deleted.
Check Facility Code in HID Mode | Checks the facility code of a HID card.
Facility Code | Enters the facility code of a HID card. When you tap the [Store] key, the facility code is stored.

Back to top