# ADDING A REGISTERED IMAGE TO AN ORIGINAL (CUSTOM IMAGE)

## Overview

This function adds an image registered in the machine to an original to make a copy. An image must be registered from the printer driver to the machine. See "REGISTERING A CUSTOM IMAGE".

- A custom image is printed with the registered size. The size remains unchanged even when the copy ratio is enlarged or reduced.
- A different custom image cannot be specified for each page.

Combination of custom image with other functions

Other functions | Custom image operations
--- | ---
Margin Shift | The margin range is shifted before printing.
Dual Page Copy | A custom image is printed by sheet.
Covers/Inserts | Based on the custom image settings.
2in1 | A custom image isprinted for each set of pages.
Tab Copy | A custom image isprinted regardless of image shift setting.
Card shot | A custom image is printed by sheet.
Mirror Image | A custom image is printed without mirror image reverse.
B/W Reverse | A custom image is printed without B/W reverse. However, the following condition is set when printed on a dark background. Custom stamp: Printed in white Custom watermark: Printed without being whitened
Centring | A custom image is printed without centring.
Stamp menu | A custom image is printed on the stamp menu.
Photo Repeat | Cannot be combined
Multi-Page Enlargement | Cannot be combined
Hidden Pattern Print | A custom image is printed under a hidden pattern print.
Repeat Layout | Cannot be combined
Position Image | A custom image is printed at the original position regardless of the position image setting.
Book Divide | A custom image is printed by sheet.
Tandem Copy | A custom image is printed when the custom image with the same file name is registered in both the master and slave machines. If the custom image is not registered, it will be copied instead of printed.

## Operation

1. #### Place an original, and tap the [Preview] key

   Place the original in the automatic document feeder or on the document glass.
   - AUTOMATIC DOCUMENT FEEDER
   - DOCUMENT GLASS

2. #### Tap the [Others] key, and tap the [Custom Image] key

3. #### Tap the [Custom Stamp] or [Custom Watermark] key

4. #### Tap the [Image] key and select an image

   Select the required thumbnail image(s) from the available selection.

5. #### Set [Print Page] or [Original]

   For the settings, see the following "Custom image settings".
   After the settings are completed, tap and the [Back] key in sequence.

   ###### To cancel the custom image setting:

   Tap the [Off] key.

6. #### Check the preview image in the preview screen

   ###### To cancel all settings:

   Tap the [CA] key.

7. #### Tap the [Start] key to start copying

   ###### To make two or more sets of copies:

   Tap the copies display key to specify the number of copies.

### Custom image settings

For custom stamp

Description | Description
--- | ---
Print Page | Specify a page(s) for printing. First Page or All Pages
Print Position | Specify a position for printing.
Originals | ORIGINAL ORIENTATION | Specify the original orientation.
2-Sided Original Type | Specify the binding edge for a 2-sided original. Select Book or Tablet.
Angle | Specify the corner of the image. Select from 0 degrees, -90 degrees, 90 degrees, and 180 degrees.

For custom watermark

Description | Description
--- | ---
Print Pattern | Transparent: Makes an original image transparent for stamp copy. Overlap: Hides a watermark added to an original image for stamp copy.
Exposure | Select the exposure from nine levels.
Print Page | Select First Page or All Pages.
Print Position | Specify a position for stamp copy.
Originals | ORIGINAL ORIENTATION | Specify the original orientation.
2-Sided Original Type | Specify the binding edge for a 2-sided original. Select Book or Tablet.
Angle | Select from 0 degrees, -90 degrees, 90 degrees, and 180 degrees.

Back to top