# SYSTEM SETTINGS LIST

## Overview

The following is a list of setting mode items, factory default settings and restrictions for each item.
Depending on the machine specifications and peripheral devices installed, it may not be possible to use some settings.

### TOTAL COUNT

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
TOTAL COUNT | - | Yes | Yes

### Default Settings

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Default Settings
| Yes | Yes
| Clock Adjust
| Yes | Yes
| Specify Time Zone
| - | Yes | Yes
| Date&Time Settings
| - | Yes | Yes
| Synchronize with Internet Time Server
| Disable | Yes | Yes
Daylight Saving Time Setting | Disable | Yes | Yes
Date Format | [MM/DD/YYYY] [/] [Last] [24-Hour] | Yes | Yes
| Keyboard Select
| English (US) | Yes | Yes

### List Print (User)

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| List Print (User)
| Yes | Yes
| All Custom Setting List
| - | Yes | Yes
| Printer Test Page
| - | Yes | Yes
| Sending Address List
| - | Yes | Yes
| Document Filing Folder List
| - | Yes | Yes
| Paper Setting List
| - | Yes | Yes

### Paper Tray Settings

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Paper Tray Settings
| Yes | Yes
| Auto Switching of Tray
| Enable | Yes | Yes
| Tray 1
| Plain, 8-1/2" × 11" | Yes | Yes
| Tray 2
| Plain, 8-1/2" × 11" | Yes | Yes
| Tray 3
| Plain, Auto-AB | Yes | Yes
| Tray 4
| Yes | Yes
| Tray 5*1, 2
| Plain, 8-1/2"*1 Tray5-Plain, Auto-AB*2 | Yes | Yes
| Tray 6*2
| Plain, Auto-AB | Yes | Yes
| Tray 7*3
| Plain, Auto-AB | Yes | Yes
| Tray 8*3
| Plain, Auto-AB | Yes | Yes
| Bypass*4
| Plain, Auto-AB | Yes | Yes
| Inserter (Upper)
| Plain, Auto-AB | Yes | Yes
| Inserter (Lower)
| Plain, Auto-AB | Yes | Yes
| Custom Size Registration (Bypass)
| Custom 1 to 7: X=17" Y=11" | Yes | Yes

*1 When a large capacity tray (MX-LC12) is installed
*2 When the large capacity trays are installed
*3 When two large capacity trays are installed
*4 When a bypass tray is installed

### Paper Type Registration

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Paper Type Registration
| - | Yes | Yes

### Printer Condition Settings

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Printer Condition Settings
| Yes | Yes
| Default Settings
| Yes | Yes
| Copies
| 1 sets of copies | Yes | Yes
| Orientation
| Portrait | Yes | Yes
| Default Paper Size
| A4 (8-1/2" × 11") | Yes | Yes
| Default Output Tray
| Varies depending on the machine configuration | Yes | Yes
| Default Paper Type
| Plain paper | Yes | Yes
| Initial Resolution Settings
| 600 dpi (High Quality) | Yes | Yes
| Disable Blank Page Print
| Disable | Yes | Yes
| Line Thickness
| 5 | Yes | Yes
| 2-Sided Print
| 1-Sided | Yes | Yes
| N-Up Print
| 1-Up | Yes | Yes
| Fit To Page
| Enable | Yes | Yes
| OUTPUT
| Varies depending on the machine configuration | Yes | Yes
| Print per Unit
| Enable | Yes | Yes
| Separator Page
| Disabled | Yes | Yes
| Staple Position
| Disabled | Yes | Yes
| Punch
| Disable | Yes | Yes
| Fold
| Disable | Yes | Yes
| Saddle Fold
| Inside | Yes | Yes
| Z-Fold Paper Size
| All Enabled | Yes | Yes
| C-Fold
| Print Side: Inside Fold Orientation: Open Right | Yes | Yes
| Accordion Fold
| Fold Orientation: Open Right | Yes | Yes
| Double Fold
| Print Side: Inside Fold Orientation: Open Right | Yes | Yes
| Half Fold
| Print Side: Inside | Yes | Yes
| Trimming Width Settings
| 2.0 mm | Yes | Yes
| QUICK FILE
| Disable | Yes | Yes
| PCL Settings
| Yes | Yes
| PCL Symbol Set Setting
| PC-8 | Yes | Yes
| PCL Font Setting
| Internal Font, 0: Courier | Yes | Yes
| PCL Line Feed Code
| 0.CR=CR; LF=LF; FF=FF | Yes | Yes
| Wide A4
| Disable | Yes | Yes
| PostScript Settings
| Yes | Yes
| Print PS Error
| Disable | Yes | Yes
| Binary Processing
| Disable | Yes | Yes

### Document Filing Control

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Document Filing Control
| - | Yes | Yes

### USB-Device Check

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| USB-Device Check
| - | Yes | Yes
| Recognized Device
| - | Yes | Yes
| Driver
| - | Yes | Yes

### Operation Settings

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Operation Settings
| No | Yes
| Enlarge Display Mode
| Disable | No | Yes
| Keys Touch Sound
| Middle | No | Yes
| Key Touch Sound at Initial Point
| Disable | No | Yes
| Auto Clear Setting
| 60 seconds | No | Yes
| Cancel Timer
| Disable | No | Yes
| Message Time Setting
| 6 seconds | No | Yes
| MFP Display Language Setting
| American English | No | Yes
| Default Display Settings
| Home Screen | No | Yes
| Display Favourite Menus as Default
| Disable | No | Yes
| Display Action Panel as default
| Enable | No | Yes
| Disabling of Job Priority Operation
| Disable | No | Yes
| Disabling of Bypass Printing
| Disable | No | Yes
| Switch the Number of Sets to be Displayed for Job Management
| Remaining Sets | No | Yes
| Key Operation Setting
| 0.0 seconds | No | Yes
| Disable Auto Key Repeat
| Disable | No | Yes
| Time for Accepting Key Entry of Long Touch
| 0.5 seconds | No | Yes
| Double Tap Interval Setting
| 0.5 seconds | No | Yes
| Disabling of Clock Adjustment
| Disable | No | Yes
| Disabling of Covers/Inserts Mode
| Disable | No | Yes
| Disable Manual Finishing
| Disable | No | Yes
| Set Keyboard Priority*1
| External Keyboard*1 | No | Yes
| Display current path in System Settings
| Enable | No | Yes
| Enable link of current path
| Enable | No | Yes
| Initial Original Count Setting
| All Invalid | No | Yes
| Unify 10-key number in ascending order from upper left
| Disable | No | Yes
| MFP Display Pattern Setting
| Pattern 4 | No | Yes
| Preview Setting
| No | Yes
| Default List/Thumbnail Display
| No | Yes
| File Retrieve of Document Filing
| No | Yes
| Main Folder/Quick File Folder
| List | No | Yes
| Custom Folder
| List | No | Yes
| Remote Operation Settings
| No | Yes
| Remote Software Operation
| No | Yes
| Operational Authority
| Prohibited | No | Yes
| View Password Entry Screen
| Display in Both PC and MFP | No | Yes
| Operation from Specified PC
| No | Yes
| Operational Authority
| Prohibited | No | Yes
| Hostname or IP Address of PC
| - | No | Yes
| View Password Entry Screen
| Display in Both PC and MFP | No | Yes
| Operation by User Who Has Password
| No | Yes
| Operational Authority
| Prohibited | No | Yes
| View Password Entry Screen
| Display in Both PC and MFP | No | Yes
| Cookie Settings
| Not hold Cookie | No | Yes
| Soft Keyboard Template Setting
| - | No | Yes
| Customize Key Setting*2
| - | No | Yes
| Mode Key Display Setting
| - | No | Yes
| Home Screen Settings*2
| - | No | Yes

*1 When an external keyboard is not installed: Soft Keyboard
*2 This cannot be set on the machine. It can be set in Setting mode (Web version). (Administrator rights are required.)

### Device Control

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Device Control
| No | Yes
| Original Size Detector Setting
| No | Yes
| Original Detection Size Combination
| Inch-1 | No | Yes
| Cancel Detection at Document Glass
| Disable | No | Yes
| Disabling of Document Feeder
| Disable | No | Yes
| Original Feeding Mode
| All Disabled | No | Yes
| Disabling of Duplex
| Disable | No | Yes
| Disabling of Large Capacity Cassette*1
| Disable | No | Yes
| Disabling of Tray Settings
| Disable | No | Yes
| Disabling of Bypass-Tray*3
| Disable | No | Yes
| Disabling of Inserter*4
| Disable | No | Yes
| Disabling of Offset*2
| Disable | No | Yes
| Disabling of Stapler*2
| Disable | No | Yes
| Automatic Saddle Stitch*5
| Enable | No | Yes
| Saddle Stitch Position Fine Adjust*5
| All 0 mm | No | Yes
| Saddle Stitch Position Adjust*6
| 0 | No | Yes
| Disabling of Punch*7
| Disable | No | Yes
| Disabling of Folding Unit*8
| Disable | No | Yes
| Disabling of Trimming Module*9
| Disable | No | Yes
| Disabling of Stacker 1*10
| Disable | No | Yes
| Disabling of Stacker 2*11
| Disable | No | Yes
| Auto Paper Selection Setting
| Plain | No | Yes
| Stacker Settings*10
| No | Yes
| Stack Setting for Additional Jobs*10
| Not Allowed | No | Yes
| Auto Switching Setting*11
| No | No | Yes
| Tandem Connection Setting
| No | Yes
| IP Address of Client Machine
| 0.0.0.0 | No | Yes
| Port Number
| 50001 | No | Yes
| Disabling of Master Machine Mode
| Disable | No | Yes
| Disabling of Client Machine Mode
| Disable | No | Yes
| Detect Standard in Auto Colour Mode
| 3(Normal) | No | Yes
| Double Feed Detection Setting
| Enable | No | Yes
| Auto Switching of Finisher Trays*2
| Enable | No | Yes
| Optimization of a Hard Disk
| - | No | Yes
| Fusing Cleaning Mode
| - | No | Yes
| MC Cleaning Mode
| - | No | Yes
| Fusing Control Settings
| No | Yes
| Paper Weight
| 60 - 89 g/m2 | No | Yes
| List Print
| One Sided | No | Yes
| Black Streak Reduction
| Disable | No | Yes
| Status Indicator Setting*12
| - | No | Yes
| Display warning message for black streaks detection.
| Disable | No | Yes

*1 When a large capacity tray is installed
*2 When a saddle finisher or finisher is installed
*3 When the bypass tray is installed
*4 When the inserter is installed
*5 When the saddle finisher is installed
*6 When the saddle finisher (100-sheet stapling) is installed
*7 When the punch module is installed
*8 When the folding unit is installed
*9 When the trimming module is installed
*10 When the stacker is installed
*11 When two stackers are installed
*12 When the status indicator is installed

### Copy Function Settings

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Copy Function Settings
| No | Yes
| Initial Status Settings
| No | Yes
| Paper Tray
| Varies depending on the machine configuration | No | Yes
| Exposure Type
| Auto | No | Yes
| Copy Ratio
| 100% | No | Yes
| 2-Sided Copy
| 1-Side to 1-Side | No | Yes
| OUTPUT
| Varies depending on the machine configuration | No | Yes
| Copy Function Settings
| No | Yes
| Copy Exposure Adjustment
| Document Glass: 5(Normal) Document Feeder: 5(Normal) | No | Yes
| Rotation Copy Setting
| Rotation copy | No | Yes
| Add or Change Extra Preset Ratios
| - | No | Yes
| Setting a Maximum Number of Copies
| 9999 | No | Yes
| Initial Margin Shift Setting
| No | Yes
| Side 1
| 1/2" | No | Yes
| Side 2
| 1/2" | No | Yes
| Erase Width Adjustment
| No | Yes
| Edge Clearance Width
| 1/2" | No | Yes
| Center Clearance Width
| 1/2" | No | Yes
| Card Shot Settings
| No | Yes
| Original Size
| X: 3-3/8", Y: 2-1/8" | No | Yes
| Fit to Page
| Disable | No | Yes
| Automatic Saddle Stitch*
| Enable | No | Yes
| Initial Tab Copy Setting
| 1/2" | No | Yes
| Disable Registration of Program
| Disable | No | Yes
| Disabling of Bypass-Tray in Duplex Copy
| Disable | No | Yes
| Disabling of Auto Paper Selection
| Disable | No | Yes
| Auto Selection Setting of Tray that is Supplied the Paper
| Disable | No | Yes
| Disabling Registration of Custom Image
| Disable | No | Yes
| Disabling sending while copying
| Disable | No | Yes
| 600 dpi × 600 dpi Scanning Mode for Document Feeder
| Disable | No | Yes
| Quick Scan from Document Glass
| Enable | No | Yes
| Auto Clear Before Copy Job Execution
| Disable | No | Yes
| Auto Calibration
| No | Yes
| Auto Calibration
| - | No | Yes

* When a saddle finisher installed

### Printer Settings

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Printer Settings
| No | Yes
| Condition Settings
| No | Yes
| Prohibit Notice Page Printing
| Enable | No | Yes
| Prohibit Test Page Printing
| Disable | No | Yes
| A4/Letter Size Auto Change
| Disable | No | Yes
| Print Density Level
| 3(Normal) | No | Yes
| Bypass Tray Settings*
| No | Yes
| Enable Detected Paper Size in Bypass Tray
| Disable | No | Yes
| Enable Selected Paper Type in Bypass Tray
| Enable | No | Yes
| Exclude Bypass-Tray from Auto Paper Select
| Disable | No | Yes
| Job Spool Queuing
| Enable | No | Yes
| Disabling of USB Memory Direct Print
| Disable | No | Yes
| Disabling of Network Folder Direct Print
| Disable | No | Yes
| Disabling sending while printing
| Disable | No | Yes
| Interface Settings
| No | Yes
| Hexadecimal Dump Mode
| Disable | No | Yes
| I/O Timeout
| 60 seconds | No | Yes
| Enable USB Port
| Enable | No | Yes
| USB Port Emulation Switching
| Auto | No | Yes
| Enable Network Port
| Enable | No | Yes
| Network Port Emulation Switching
| Auto | No | Yes
| Port Switching Method
| Switch at End of Job | No | Yes
| Auto Calibration
| - | No | Yes

* When the bypass tray is installed

### Image Send Settings

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Image Send Settings
| No | Yes
| Operation Settings
| No | Yes
| Default Settings
| No | Yes
| Hold settings for a while after scanning has been completed.
| Disable | No | Yes
| Default Display Settings
| E-mail | No | Yes
| Address Book Default Selection
| No | Yes
| Apply Addresses of Sending Modes Only
| Enable | No | Yes
| Category to be Displayed as Default
| None | No | Yes
| Display all address type regardless of the mode being displayed currently.
| Disable | No | Yes
| Enlarge the Address Book
| Enable | No | Yes
| Image Orientation
| Portrait | No | Yes
| Initial Resolution Setting
| No | Yes
| Scan
| Apply the Resolution Set when Stored: Disable, 200 × 200 dpi | No | Yes
| E-mail
| Apply the Resolution Set when Stored: Disable, 200 × 200 dpi | No | Yes
| Default Exposure Settings
| Auto | No | Yes
| Default Original Image Type
| Text | No | Yes
| Sharpness
| 3 (Normal) | No | Yes
| Contrast
| 3 (Normal) | No | Yes
| Must Input Next Address Key at Broadcast Setting
| Disable | No | Yes
| Scan Complete Sound Setting
| Middle | No | Yes
| Disable Switching of Display Order
| Disable | No | Yes
| Default Verification Stamp*1
| Disable | No | Yes
| Erase Width Adjustment
| No | Yes
| Edge Clearance Width
| 1/2" | No | Yes
| Center Clearance Width
| 1/2" | No | Yes
| Time Specified Output of Received Data
| Disable | No | Yes
| Enable/Disable Settings
| No | Yes
| Settings to Disable Registration
| No | Yes
| Disable Registering Destination from Operation Panel
| All Invalid | No | Yes
| Disable Registering Destination on Web Page*4
| All Invalid | No | Yes
| Disable All Program Item Registration
| Disable | No | Yes
| Disable Destination Registration Using Global Address Search*4
| All Invalid | No | Yes
| Disable Registering Using Network Scanner Tool*4
| Disable | No | Yes
| Disabling of Forwarding via Network
| Disable | No | Yes
| Settings to Disable Transmission
| No | Yes
| Disable Selection from Address Book
| All Invalid | No | Yes
| Disable Direct Entry
| All Invalid | No | Yes
| Own Name and Destination Set
| No | Yes
| Sender Data Registration
| - | No | Yes
| Registration of Own Name Select
| - | No | Yes
| Scan Settings
| No | Yes
| Scan Settings
| No | Yes
| Default Sender Set
| - | No | Yes
| Default Colour Mode Settings
| No | Yes
| Scanner Common
| (No item)
| Auto | No | Yes
| (No item)
| Greyscale | No | Yes
| Disable Change of B/W Setting in Auto Mode
| Disable | No | Yes
| Common to e-mails
| (No item)
| Auto | No | Yes
| (No item)
| Greyscale | No | Yes
| Disable Change of B/W Setting in Auto Mode
| Disable | No | Yes
| Initial File Format Setting
| Scanner Common
| No | Yes
| File Format
| PDF | No | Yes
| Black & White
| MMR (G4) | No | Yes
| Colour/Greyscale
| Middle | No | Yes
| Bk Letter Emphasis
| Disable | No | Yes
| Specified Pages per File
| Disable | No | Yes
| Number of Pages
| 1 | No | Yes
| E-mail
| No | Yes
| File Format
| PDF | No | Yes
| Black & White
| MMR (G4) | No | Yes
| Colour/Greyscale
| Middle | No | Yes
| Specified Pages per File
| Disable | No | Yes
| Number of Pages
| 1 | No | Yes
| Compression Mode at Broadcasting
| No | Yes
| Black & White
| MH (G3) | No | Yes
| Colour/Greyscale
| Middle | No | Yes
| Bk Letter Emphasis
| Disable | No | Yes
| Maximum Size of E-mail Attachments
| Unlimited | No | Yes
| Maximum Size of E-mail Attachments (FTP/Network Folder)
| Unlimited | No | Yes
| Bcc Setting
| No | Yes
| Enable Bcc
| Disable | No | Yes
| Display Bcc Address on the Job Management Screen
| Disable | No | Yes
| Disable Scan Function
| No | Yes
| PC Scan
| Disable | No | Yes
| Default Address Setting
| Disable | No | Yes

*3 When the verification stamp unit is installed
*4 When the network connection is enabled

### Document Filing Settings

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Document Filing Settings
| No | Yes
| Default Mode Settings
| Sharing Mode | No | Yes
| Sort Method Setting
| Date | No | Yes
| Administrator Authority Setting
| No | Yes
| Delete File
| Disable | No | Yes
| Delete Folder
| Disable | No | Yes
| Change Password
| Disable | No | Yes
| Delete All Quick Files
| No | Yes
| Delete Now
| - | No | Yes
| Delete quick files at power up
| Enable | No | Yes
| Image Orientation
| Portrait | No | Yes
| Default Colour Mode Settings
| Auto | No | Yes
| Default Exposure Settings
| Auto | No | Yes
| Default Original Image Type
| Text | No | Yes
| Initial Resolution Settings
| 600 × 600 dpi | No | Yes
| Scan Complete Sound Setting
| Middle | No | Yes
| Default Output Tray
| Varies depending on the machine configuration | No | Yes
| Disabling Text/Stamp printing at Reprint
| Disable | No | Yes
| Batch Print Settings
| No | Yes
| Selection of [All Users] is not allowed
| Enable | No | Yes
| Selection of [User Unknown] is not allowed.
| Enable | No | Yes
| Erase Width Adjustment
| No | Yes
| Edge Clearance Width
| 1/2" | No | Yes
| Center Clearance Width
| 1/2" | No | Yes
| Card Shot Settings
| No | Yes
| Original Size
| X: 3-3/8", Y: 2-1/8" | No | Yes
| Fit to Store Size
| Disable | No | Yes
| Setting of store/delete after file print
| Store | No | Yes
| Scan to External Memory Device Setting
| No | Yes
| Default Colour Mode Settings
| Auto | No | Yes
| Initial File Format Setting
| PDF | No | Yes
| Black & White
| MMR (G4) | No | Yes
| Colour/Greyscale
| No | Yes
| Compression Ratio
| Middle | No | Yes
| Bk Letter Emphasis
| Disable | No | Yes
| Specified Pages per File
| Disable | No | Yes
| Default Exposure Settings
| Auto | No | Yes
| Default Original Image Type
| Text | No | Yes
| Initial Resolution Settings
| 200 × 200 dpi | No | Yes
| Disable Storing to External Memory Device
| Disable | No | Yes
| Default Setting of PDF Format for PC Browsing
| No | Yes
| Black & White
| No | Yes
| Compression Mode
| MMR (G4) | No | Yes
| Colour/Greyscale
| No | Yes
| Compression Ratio
| Middle | No | Yes
| Copy
| Disable | No | Yes
| Apply the resolution at job execution
| Disable | No | Yes
| PRINTER
| Disable | No | Yes
| Apply the resolution at job execution
| Disable | No | Yes
| Scan to
| Disable | No | Yes
| Apply the resolution at job execution
| Disable | No | Yes
| Scan to HDD
| Disable | No | Yes
| Apply the resolution at job execution
| Disable | No | Yes
| Document Output Options
| No | Yes
| Print
| No | Yes
| Copy
| Enable | No | Yes
| PRINTER
| Enable | No | Yes
| Scan Send
| Disable | No | Yes
| Scan to HDD
| Enable | No | Yes
| Scan Send
| No | Yes
| Copy
| Disable | No | Yes
| PRINTER
| Disable | No | Yes
| Scan Send
| Enable | No | Yes
| Scan to HDD
| Enable | No | Yes
| Automatic Deletion of File Settings
| All Invalid | No | Yes

### List Print (Administrator)

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| List Print (Administrator)
| No | Yes
| Administrator Settings List
| - | No | Yes
| Image Sending Activity Report
| - | No | Yes
| Data Receive/Forward List
| - | No | Yes
| Web Settings List*1
| - | No | Yes
| Metadata Set List*2
| - | No | Yes

*1 When the network is enabled
*2 When the application integration module is installed

### Sharp OSA Settings

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Sharp OSA Settings
| No | Yes
| External Account Setting*1
| No | Yes
| External Account Control
| Disable | No | Yes
| Enable Authentication by External Server
| Disable | No | Yes
| USB Driver Settings*2
| No | Yes
| External Keyboard
| Use Internal Driver | No | Yes
| Card Reader/Writer
| Use Internal Driver | No | Yes
| USB Memory
| Use Internal Driver | No | Yes
| Level of Encryption
| None | No | Yes
| Job Priority Preference
| - | No | Yes

*1 When an external account module is installed
*2 When an external account module or application communication module is installed

### Enable/Disable Settings

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| ENABLE / DISABLE SETTINGS
| No | Yes
| Printer Condition Settings
| No | Yes
| Disable Blank Page Print
| Disable | No | Yes
| User Control
| No | Yes
| Disabling of Printing by Invalid User
| Disable | No | Yes
| Operation Settings
| No | Yes
| Cancel Auto Clear Timer
| Disable | No | Yes
| Disabling of Job Priority Operation
| Disable | No | Yes
| Disabling of Bypass Printing
| Disable | No | Yes
| Disable Auto Key Repeat
| Disable | No | Yes
| Disabling of Clock Adjustment
| Disable | No | Yes
| Disabling of Covers/Inserts Mode
| Disable | No | Yes
| Disable Manual Finishing*1
| Disable | No | Yes
| Device Control
| No | Yes
| Disabling of Document Feeder
| Disable | No | Yes
| Disabling of Duplex
| Disable | No | Yes
| Disabling of Large Capacity Cassette*2
| Disable | No | Yes
| Disabling of Tray Settings
| Disable | No | Yes
| Disabling of Bypass-Tray*3
| Disable | No | Yes
| Disabling of Inserter*1
| Disable | No | Yes
| Disabling of Offset*4
| Disable | No | Yes
| Disabling of Stapler*4
| Disable | No | Yes
| Disabling of Punch*5
| Disable | No | Yes
| Disabling of Folding Unit*6
| Disable | No | Yes
| Disabling of Trimming Module*7
| Disable | No | Yes
| Disabling of Stacker 1*8
| Disable | No | Yes
| Disabling of Stacker 2*9
| Disable | No | Yes
| Disabling of Master Machine Mode
| Disable | No | Yes
| Disabling of Client Machine Mode
| Disable | No | Yes
| Copy Function Settings
| No | Yes
| Disable Registration of Program
| Disable | No | Yes
| Disabling of Bypass-Tray in Duplex Copy
| Disable | No | Yes
| Disabling of Auto Paper Selection
| Disable | No | Yes
| Disabling Registration of Custom Image
| Disable | No | Yes
| Disabling sending while copying
| Disable | No | Yes
| Printer Settings
| No | Yes
| Prohibit Notice Page Printing
| Enable | No | Yes
| Prohibit Test Page Printing
| Disable | No | Yes
| Exclude Bypass-Tray from Auto Paper Select
| Disable | No | Yes
| Disabling of USB Memory Direct Print
| Disable | No | Yes
| Disabling of Network Folder Direct Print
| Disable | No | Yes
| Disabling sending while printing
| Disable | No | Yes
| Image Send Settings
| No | Yes
| Disable Switching of Display Order
| Disable | No | Yes
| Settings to Disable Registration
| No | Yes
| Disable Registering Destination from Operation Panel
| All Invalid | No | Yes
| Disable Registering Destination on Web Page*10
| All Invalid | No | Yes
| Disable Registration of Program
| No | Yes
| Disable All Program Item Registration
| Disable | No | Yes
| Disable Destination Registration Using Global Address Search*10
| All Invalid | No | Yes
| Disable Registration Using Network Scanner Tool*10
| Disable | No | Yes
| Disabling of Forwarding via Network*10
| Disable | No | Yes
| Settings to Disable Transmission
| No | Yes
| Disable Selection from Address Book
| All Invalid | No | Yes
| Disable Direct Entry
| All Invalid | No | Yes
| Disable Scan Function
| No | Yes
| PC Scan
| Disable | No | Yes
| Document Filing Settings
| No | Yes
| Disabling Text/Stamp printing at Reprint
| Disable | No | Yes
| Batch Print Settings
| No | Yes
| Selection of [All Users] is not allowed
| Enable | No | Yes
| Selection of [User Unknown] is not allowed.
| Enable | No | Yes
| Disable Storing to External Memory Device
| Disable | No | Yes
| Web Browser Settings
| No | Yes
| Disable URL Entry
| Disable | No | Yes
| Disable Additional Edit of Favourite
| Disable | No | Yes
| Disable Registration/Edit of Home Page
| Disable | No | Yes
| Disable Print from Web Browse Mode
| Disable | No | Yes
| Disable display of History
| Disable | No | Yes
| Security Settings
| No | Yes
| Hidden Pattern Print Setting
| No | Yes
| Disable Direct Entry
| Disable | No | Yes

*1 When the inserter is installed
*2 When a large capacity tray is installed
*3 When the bypass tray is installed
*4 When the saddle finisher or the finisher is installed
*5 When the punch module is installed
*6 When the folding unit is installed
*7 When the trimming module is installed
*8 When the stacker is installed
*9 When two stackers are installed
*10 When the network connection is enabled

### DATA BACKUP

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| DATA BACKUP
| No | Yes
| Storage Backup
| - | No | Yes
| Device Cloning
| - | No | Yes
| Address Book Forward
| - | No | Yes

### Product Key

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| PRODUCT KEY*
| No | Yes
| Serial Number
| - | No | Yes
| Barcode Font Kit
| - | No | Yes
| Application Integration Module
| - | No | Yes
| Application Communication Module
| - | No | Yes
| External Account Module
| - | No | Yes
| XPS expansion kit
| - | No | Yes

* It may not be possible to use some settings, depending on the peripheral devices installed.

### Storing/Calling of System Settings

U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Storing/Calling of System Settings
| No | Yes
| Restore Factory Defaults
| - | No | Yes
| Store Current Configuration
| - | No | Yes
| Restore Configuration
| - | No | Yes

Back to top