# MAKING AN INTERRUPT COPY

## Overview

When you need to make an urgent copy and the machine is busy with a long copy run or other job, you can use interrupt copy. The interrupt copy function interrupts data output and preferentially outputs an original with interrupt copy specified.

- The [Interrupt] key does not appear while an original is being scanned.
- Depending on the settings of the job in progress, the [Interrupt] key may not appear.
- Interrupt copy cannot be used in combination with the following functions:
  Job Build, Tandem Copy, Book Copy, Card Shot, Multi-Page Enlargement, Original Count, Proof Copy, Preview Setting, Book Divide
- When you place an original on the document glass, you cannot select the 2-sided copying, sort mode, or staple sort features to make an interrupt copy.
  If any of these functions are necessary, use the automatic document feeder.

## Operation

1. #### Tap the [Interrupt] key

   The interrupt mode screen appears.

   If user authentication is enabled, tap the [Interrupt] key to display the user authentication screen. Enter the user name and password to perform user authentication.

2. #### Place the original

   Place the original in the automatic document feeder or on the document glass.
   - AUTOMATIC DOCUMENT FEEDER
   - DOCUMENT GLASS

3. #### Set each copy item as required

   ###### To cancel interrupt copying:

   Tap the [Cancel] key

4. #### Tap the [Start] key to start interrupt copying

   When the interrupt copy job is completed, the interrupted job resumes.
   The interrupt copy function does not display the preview of the scanned original.

Back to top