# SKIPPING BLANK PAGES IN AN ORIGINAL (BLANK PAGE SKIP)

## Overview

If the scanned original contains blank pages, this function skips them to copy only non-blank pages.
If an original of which one side is blank is scanned, blank pages are skipped for 2-sided copying.

Depending on the original, some pages that are not blank may be detected as blank pages and thus not copied, and some pages that are blank may not be detected as blank and thus copied.

## Operation

1. #### Place an original, and tap the [Preview] key

   Place the original in the automatic document feeder or on the document glass.
   - AUTOMATIC DOCUMENT FEEDER
   - DOCUMENT GLASS

2. #### Tap the [Others] key, and tap the [Blank Page Skip] key

3. #### Tap the [Skip Blank Page] or [Skip Blank and Back Shadow] key

   After the settings are completed, tap and the [Back] key in sequence.

   ###### To cancel the blank page skip setting:

   Tap the [Off] key.

4. #### Check the preview image in the preview screen

   ###### To cancel all settings:

   Tap the [CA] key.

5. #### Tap the [Start] key

   ###### To make two or more sets of copies:

   Tap the copies display key to specify the number of copies.

6. #### Check the confirmation message, and tap the [Execute] key to start copying

   On the confirmation screen, the number of scanned original sheets appears in (A), the number of scanned sides in (B), and the number of copies excluding blank pages in (C). For example, if five original sheets that include two blank pages are scanned by duplex scanning, (A) will show "5", (B) will show "10", and (C) will show "8".

Back to top