# EXTERIOR

This section describes the names and functions of the respective parts on the exterior of the machine.
Tap the name to make its details pop up.

×
Automatic document feeder
This automatically feeds and scans multiple originals. Both sides of 2-sided originals can be automatically scanned at one time.
-AUTOMATIC DOCUMENT FEEDER
×
Front cover
Open this to remove a paper misfeed from or to switch the main power switch on and off.
×
Status indicator*
The status of the machine is indicated.
-STATUS INDICATORS
×
Operation panel
This panel hosts the [POWER] button, [Power Save] button/indicator, [Home Screen] button/indicator, main power button, USB port (A type) and touch panel. Use the touch panel to operate each of these functions.
-OPERATION PANEL
×
Punch module*
This punches and outputs paper.
×
USB connector (A type)
This is used to connect a USB device such as a USB memory device to the machine.
For the USB cable, use a shielded cable.
Supports USB 2.0 (Hi-Speed).
×
Keyboard*
Use this as a substitute for the soft keyboard displayed on the touch panel.
-NAMES AND FUNCTIONS OF SOFT KEYBOARD KEYS
×
Tray 1
Store paper in this tray. Up to 1,200 sheets can be stored.
-TRAY 1/2
×
Tray 2
Store paper in this tray. Up to 800 sheets can be stored.
-TRAY 1/2
×
Tray 3
Store paper in this tray. Up to 500 sheets can be stored.
-TRAY 3/4
×
Tray 4
Store paper in this tray. Up to 500 sheets can be stored.
-TRAY 3/4
×
Tray 5 (MX-LC12)*
Store paper in this tray. Up to 3,500 sheets can be stored.
-LARGE CAPACITY TRAY
×
Bypass tray*
Use this tray to feed paper manually.
When loading paper larger than A4R or 8-1/2" x 11"R, pull out the extension guide.
-BYPASS-TRAY
×
Trimming module*
This trims the excess of saddle-stitched output.
×
Saddle finisher (100-sheet stapling)*
This staples and folds paper.
-SADDLE FINISHER (100-SHEET STAPLING)
×
Finisher (100-sheet stapling)*
This staples and outputs paper.
-FINISHER (100-SHEET STAPLING)
×
Curl correction unit*
This corrects curls in printed paper.
×
Toner tray
This tray contains toner cartridge. When the toner in a cartridge runs out, the cartridge that ran out must be replaced.
-TONER CARTRIDGE

×
Large capacity trays*
Store paper in this tray. Up to 2,500 sheets can be stored in each tray.
-LARGE CAPACITY TRAYS
×
Bypass tray*
Use this tray to feed paper manually.
When loading paper larger than A4R or 8-1/2" x 11"R, pull out the extension guide.
×
Paper cart*
This is a cart that is installed in the high capacity stacker. It is useful when you carry a large number of output sheets.
×
Inserter*
Covers and insertion sheets to be inserted into printed sheets can be loaded.
Using the manual finishing function, you can directly feed paper into the finisher or saddle finisher to staple, punch or fold the paper.
×
Folding unit*
This folds and outputs paper.
×
High capacity stacker*
This unit is useful when you output a large number of copies. A maximum of 5,000 sheets of paper can be output.
You can also connect two units.
-HIGH CAPACITY STACKER
* Optional.
Back to top